Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A737	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G.G. Beckmann	Locality:
	Date Desc.:	19/05/60	Elevation:	 405 metres
	Map Ref.:	Sheet No. : SI54-9   1:250000	Rainfall:	711
	Northing/Long.:	138.946111111111	Runoff:	Slow
	Easting/Lat.:	-34.7319444444445	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	7 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 12.01-20m, . *Species includes - Pinus radiata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark grey (10YR4/1-Moist); ; Sandy light clay; Single grain grade of structure; Firm consistence; 
	A21	0.13 - 0.3 m	Light yellowish brown (2.5Y6/4-Moist); ; Sandy loam; Single grain grade of structure; Firm 
	consistence; 
	A22	0.3 - 0.38 m	Light yellowish brown (2.5Y6/4-Moist); ; Clayey sand; Single grain grade of structure; Firm 
	consistence; 
	B2	0.38 - 0.76 m	Brownish yellow (10YR6/6-Moist); , 2.5Y64; , 10R46; Heavy clay; Massive grade of structure; 
	Weak consistence; Moderately plastic; 
	3B	0.76 - 1.02 m	Brownish yellow (10YR6/7-Moist); , 5Y62; Heavy clay; Massive grade of structure; Very weak 
	consistence; Moderately plastic; 
	CB	1.02 - 1.14 m	; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Weak consistence; 
	C	1.22 - 1.35 m	Brownish yellow (10YR6/6-Moist); ; 
	Morphological Notes
	Observation Notes
	Site Notes
	MT CRAW.FOREST

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A737	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.8H	 0.011C	 1.5K	 0.8	 0.18	 0.11
	0.13 - 0.3	5.7H	 0.01C
	0.3 - 0.38	6H	 0.007C
	0.38 - 0.76	6.8H	 0.016C	 9.1K	 9.9	 0.83	 0.75
	0.76 - 1.02	7.2H	 0.022C
	1.02 - 1.14	7.4H	 0.023C
	1.22 - 1.35	7.1H	 0.023C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.3E	 0.009F	 0.065B	 29	 21C	 65	 8	 6
	0.13 - 0.3	 0.033B	 76	 23C	 64	 8	 6
	0.3 - 0.38
	0.38 - 0.76	 0.011F	 0.043B	 4C	 11	 4	 80
	0.76 - 1.02	 1C	 36	 14	 50
	1.02 - 1.14	 1C	 33	 23	 42
	1.22 - 1.35	 0.02F	 2C	 71	 15	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.3
	0.3 - 0.38
	0.38 - 0.76
	0.76 - 1.02
	1.02 - 1.14
	1.22 - 1.35

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A737	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded