Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1146	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	24/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6112030 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	337190  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr4.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Field pH 7.5 
	(Raupach); Sharp change to - 
	A2	0.1 - 0.2 m	Pinkish yellow (7.5YR8/2-Moist); ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 50-90%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Field pH 
	7.5 (Raupach); Sharp change to - 
	A/B	0.2 - 0.28 m	Reddish brown (5YR4/3-Moist); , 5YR56; , 7.5YR82; Sandy clay; 20-50 mm, Columnar; Very 
	firm consistence; 20-50%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Field 
	pH 7.5 (Raupach); Clear change to - 
	2B2	0.28 - 0.4 m	Yellowish red (5YR4/6-Moist); , 5YR56; Sandy clay; 20-50 mm, Columnar; Moist; Very firm 
	consistence; 20-50%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 8.5 
	(Raupach); 
	2B2	0.4 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Sandy clay; Weak grade of structure, Angular blocky; Moist; 
	Very firm consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Many (20 - 50 
	%), Calcareous, , ; Field pH 8.5 (Raupach); Gradual change to - 
	2B2k	0.5 - 0.6 m	Yellowish red (5YR5/8-Moist); ; Sandy clay; Massive grade of structure; Dry; Strong 
	consistence; 20-50%, medium gravelly, 6-20mm, Quartz, coarse fragments; Common (10 - 20 
	%), Calcareous, , Soft segregations; Field pH 9 (Raupach); 
	2B2k	0.6 - 0.7 m	Pink (7.5YR8/4-Moist); ; Massive grade of structure; Strong consistence; 20-50%, fine gravelly, 
	2-6mm, Quartz, coarse fragments; Common (10 - 20 %), Calcareous, , Soft segregations; Field 
	pH 9.5 (Raupach); Gradual change to - 
	2B3k	0.7 - 0.8 m	Reddish yellow (7.5YR6/6-Moist); ; Massive grade of structure; Dry; Strong consistence; 50-
	90%, cobbly, 60-200mm, Quartz, coarse fragments; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 9 (Raupach); 
	2R	0.8 - 1 m	Rock 
	Morphological Notes
	A2	Feldspar gravel present.
	A/B	An  A/B horizon.   SC Texture is questioned.  Feldspar gravel present.
	2B2	 SC Texture is questioned.   Feldspar gravel present.

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1146	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	2B2	 SC Texture is questioned.  Feldspar gravel present.
	2B2k	 SC Texture is questioned.  Feldspar gravel present.
	2B2k	Mica flakes present.
	2B3k	Migmatite fragments present.
	2R	Weakly foliated coarse grained quartz, muscavite and feldspar.  80% weathering 
	migmatite.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1146	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	7A	<0.06A	4.7K	0.59	0.26	0.16	8J	2.00
	0.1 - 0.2
	0.2 - 0.28	8.6A	0.12A	9.2K	6.7	0.6	1.3	20J	6.50
	0.28 - 0.4	8.7A	0.11A	11K	9.8	0.8	2.2	29J	7.59
	0.4 - 0.5
	0.5 - 0.6	9.6A	0.31A	11.7K	9.4	0.35	3.2	26J	12.31
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	<0.1C	3I	45	3	2
	0.1 - 0.2
	0.2 - 0.28	0.11C	4I	31	4	28
	0.28 - 0.4	<0.1C	3I	21	3	40
	0.4 - 0.5
	0.5 - 0.6	6.2C	4I	16	4	28
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.1 - 0.2
	0.2 - 0.28
	0.28 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1146	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded