Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	27/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6110110 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	334220  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.53
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.07 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Massive grade of structure; Dry; Very weak 
	consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 6.5 (Raupach); Sharp 
	change to - 
	A1	0.07 - 0.19 m	Reddish brown (5YR4/3-Moist); ; Loamy sand; Massive grade of structure; Dry; Very firm 
	consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 8 (Raupach); Gradual 
	change to - 
	B2k	0.19 - 0.33 m	Yellowish red (5YR5/8-Moist); ; Sandy clay; Massive grade of structure; Strong consistence; 
	Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); Gradual change to - 
	B2k	0.33 - 0.5 m	Reddish yellow (7.5YR6/6-Moist); , 10YR66; , 10YR81; Light clay; Massive grade of structure; 
	Very firm consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	C1k	0.5 - 0.85 m	Light grey (5Y7/2-Moist); , 5YR66; , 10YR81; Sandy clay; Massive grade of structure; Very firm
	 consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	C1k	0.85 - 1 m	Pale yellow (5Y7/3-Moist); , 2.5YR36; , 10YR56; Sandy clay; Massive grade of structure; 
	Strong consistence; Many (20 - 50 %), Calcareous, , ; Field pH 9 (Raupach); 
	C2k	1 - 1.6 m	Light grey (5Y7/2-Moist); , 2.5YR36; , 10YR56; Sandy clay; Massive grade of structure; Strong 
	consistence; Few (2 - 10 %), Calcareous, , ; Field pH 9 (Raupach); 
	C3	1.6 - 2.6 m	Yellowish brown (10YR5/6-Moist); , 2.5YR58; Fine sandy loam; Massive grade of structure; 
	Strong consistence; Very few (0 - 2 %), Calcareous, , ; Very few (0 - 2 %), Ferruginous, , 
	Nodules; Field pH 9 (Raupach); 
	C3	2.6 - 3.6 m	Light grey (5Y7/2-Moist); , 2.5YR36; , 10YR56; Fine sandy loam; Massive grade of structure; 
	Very firm consistence; Field pH 9 (Raupach); 
	Morphological Notes
	B2k	SC texture is uncertain.
	C1k	SC texture is uncertain.
	C1k	Tranisition zone: carbonate to parilla sand.  SC texture is uncertain.
	C2k	Moderately indurated.  SC texture is uncertain.
	C3	Moderately indurated.
	C3	Moderately indurated.

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Notes
	Observation Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	7.9A	0.13A	5.7K	1.1	0.88	0.14
	0.07 - 0.19
	0.19 - 0.33	8.9A	0.12A	10.1K	5.5	1.2	0.35
	0.33 - 0.5
	0.5 - 0.85	9.9A	0.31A	3.4K	5.9	0.81	2.4
	0.85 - 1
	1 - 1.6	9.9A	0.5A	2.2K	3.5	0.56	4.4
	1.6 - 2.6
	2.6 - 3.6	8.9A	2.18A	1.6K	2.3	0.45	2.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	0.16C	1I	43	1	8
	0.07 - 0.19
	0.19 - 0.33	14C	2I	26	2	27
	0.33 - 0.5
	0.5 - 0.85	20C	1I	23	1	29
	0.85 - 1
	1 - 1.6	3.7C	1I	50	1	28
	1.6 - 2.6
	2.6 - 3.6	0I	68	0	25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.19
	0.19 - 0.33
	0.33 - 0.5
	0.5 - 0.85
	0.85 - 1
	1 - 1.6
	1.6 - 2.6
	2.6 - 3.6

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded