Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1154	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	27/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6108830 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	336240  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Sand; Massive grade of structure; Loose consistence; Field 
	pH 7 (Raupach); Gradual change to - 
	A2	0.1 - 0.42 m	White (10YR8/1-Moist); ; Sand; Massive grade of structure; Loose consistence; Field pH 7.5 
	(Raupach); Sharp change to - 
	A2	0.42 - 0.64 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; Massive grade of structure; Firm consistence; 
	Field pH 7.5 (Raupach); 
	A2	0.64 - 0.9 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; Massive grade of structure; Firm consistence; 
	Field pH 8 (Raupach); 
	A2	0.9 - 1.1 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; Massive grade of structure; Strong 
	consistence; Few (2 - 10 %), Calcareous, , ; Field pH 8 (Raupach); 
	Ck	1.1 - 1.5 m	Yellow (10YR7/6-Moist); ; Sand; Massive grade of structure; Very weak consistence; Few (2 -
	 10 %), Calcareous, , ; Field pH 9 (Raupach); 
	Ck	1.5 - 2 m	Yellow (10YR7/6-Moist); ; Sand; Massive grade of structure; Very weak consistence; Few (2 -
	 10 %), Calcareous, , ; Field pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1154	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7A	<0.06A	1.4K	0.36	0.09	0.1
	0.1 - 0.42	8.2A	<0.06A	0.51K	0.16	0.15	0.38
	0.42 - 0.64
	0.64 - 0.9	8.2A	<0.06A	3K	1.8	0.42	0.56
	0.9 - 1.1
	1.1 - 1.5	9.3A	<0.06A	3.7K	1.5	0.33	0.82
	1.5 - 2
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	<0.1C	0I	49	0	0
	0.1 - 0.42	<0.1C	0I	54	0	2
	0.42 - 0.64
	0.64 - 0.9	<0.1C	2I	42	2	4
	0.9 - 1.1
	1.1 - 1.5	2C	1I	53	1	7
	1.5 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.42
	0.42 - 0.64
	0.64 - 0.9
	0.9 - 1.1
	1.1 - 1.5
	1.5 - 2

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1154	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded