Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	27/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6112280 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	334720  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR4/2-Moist); ; Sand; Massive grade of structure; Loose consistence; Field pH 7 
	(Raupach); Clear change to - 
	A2	0.08 - 0.14 m	Very pale brown (10YR8/3-Dry); ; Sand; Massive grade of structure; Loose consistence; Field 
	pH 6.5 (Raupach); Sharp change to - 
	A/B2	0.14 - 0.22 m	Brown (7.5YR5/4-Moist); , 7.5YR76; , 2.5YR68; Sandy clay; 50-100 mm, Columnar; Very strong
	 consistence; Field pH 7.5 (Raupach); 
	B1t	0.22 - 0.31 m	Brown (7.5YR5/4-Moist); , 2.5YR56; , 10YR76; Sandy clay; Moderate grade of structure, 
	Angular blocky; Strong consistence; Field pH 8.5 (Raupach); 
	B2t	0.31 - 0.4 m	Brown (7.5YR5/4-Moist); , 2.5YR56; , 10YR76; Sandy clay; Moderate grade of structure, 
	Angular blocky; Strong consistence; Field pH 8.5 (Raupach); Gradual change to - 
	B2tk	0.4 - 0.5 m	Reddish yellow (7.5YR7/6-Moist); , 7.5YR84; Medium clay; Moderate grade of structure, Platy; 
	Dry; Very strong consistence; 20-50%, coarse fragments; Field pH 9 (Raupach); 
	B2c	0.5 - 0.7 m	Reddish yellow (7.5YR6/6-Moist); , 5YR54; Medium clay; 2-5 mm, Platy; Dry; Very strong 
	consistence; 20-50%, coarse fragments; Field pH 9 (Raupach); 
	B2tk	0.7 - 0.9 m	Reddish yellow (7.5YR7/6-Moist); , 5YR56; , Platy; Dry; Very strong consistence; 20-50%, 
	coarse fragments; Field pH 9 (Raupach); 
	B2tk	0.9 - 1.05 m	Reddish yellow (7.5YR7/6-Moist); , 5YR54; Heavy clay; Massive grade of structure; Weak 
	grade of structure, Platy; Strong consistence; Field pH 9 (Raupach); Clear change to - 
	3C	1.05 - 1.2 m	Red (2.5YR4/6-Moist); , 10YR64; Heavy clay; Strong grade of structure, Angular blocky; Strong
	 grade of structure, 50-100 mm, Prismatic; Very strong consistence; 2-10%, fine gravelly, 2-
	6mm, subrounded, Quartz, coarse fragments; Field pH 9 (Raupach); 
	3C	1.2 - 1.5 m	Red (2.5YR4/6-Moist); , 10YR64; , 5YR56; Strong grade of structure, Angular blocky; Strong 
	grade of structure, 50-100 mm, Prismatic; Very strong consistence; 0-2%, fine gravelly, 2-6mm,
	 subrounded, Quartz, coarse fragments; Field pH 6.5 (Raupach); 
	3C	1.5 - 1.8 m	Light yellowish brown (10YR6/4-Moist); , 2.5YR46; , 5YR56; Strong grade of structure, Angular
	 blocky; Strong grade of structure, 50-100 mm, Prismatic; Very strong consistence; Field pH 6 
	(Raupach); 

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	3C	1.8 - 2.3 m	Light yellowish brown (10YR6/4-Moist); , 2.5YR46; , 5YR56; Strong grade of structure, Angular
	 blocky; Strong grade of structure, 50-100 mm, Prismatic; Very strong consistence; Field pH 6 
	(Raupach); 
	Morphological Notes
	A/B2	 An A/B horizon.  SC texture is uncertain.
	B1t	SC texture is uncertain.
	B2t	SC texture is uncertain.
	B2tk	Some clay from above persisting in pockets.
	B2tk	Pockets of Blanchetown clay appearing.
	3C	SC texture is uncertain. Fine network of former root channels.
	3C	SC texture is uncertain.
	3C	SC texture is uncertain.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.5A	0.06A	2.8K	1	0.41	0.17	6J	2.83
	0.08 - 0.14
	0.14 - 0.22	8.5A	0.09A	5.1K	6.9	1.2	2.1	16J	13.13
	0.22 - 0.31	8.8A	0.09A	5.5K	8.6	1.3	2.7	24J	11.25
	0.31 - 0.4
	0.4 - 0.5	9.5A	0.36A	7.6K	8.2	1.4	3.3	26J	12.69
	0.5 - 0.7	9.6A	0.38A	7.1K	8.1	1.4	3.6	20J	18.00
	0.7 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5	7.8A	0.55A	1.6K	8.2	1.3	6.6	22J	30.00
	1.5 - 1.8
	1.8 - 2.3
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	<0.1C	0I	41	0	4
	0.08 - 0.14
	0.14 - 0.22	<0.1C	0I	33	0	32
	0.22 - 0.31	<0.1C	1I	33	1	38
	0.31 - 0.4
	0.4 - 0.5	29C	0I	17	0	36
	0.5 - 0.7	37C	0I	14	0	33
	0.7 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5	0.13C	0I	22	0	45
	1.5 - 1.8
	1.8 - 2.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.14
	0.14 - 0.22
	0.22 - 0.31
	0.31 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.3

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded