Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	25/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6116050 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	329020  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Dry; Very weak
	 consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.5 (Raupach); 
	A1	0.1 - 0.18 m	Reddish brown (5YR4/4-Moist); , 5YR64; Loamy sand; Massive grade of structure; Dry; Very 
	weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Field 
	pH 7 (Raupach); Sharp change to - 
	B2	0.18 - 0.3 m	Dark reddish brown (5YR3/2-Moist); , 5YR44; Sandy clay; , Subangular blocky; Moderate grade
	 of structure, Prismatic; Dry; Strong consistence; Field pH 8.5 (Raupach); Gradual change to - 
	B2	0.3 - 0.4 m	Dark reddish brown (5YR3/2-Moist); , 5YR44; Light clay; Massive grade of structure; Moderate 
	grade of structure, Subangular blocky; Dry; Strong consistence; Few (2 - 10 %), Calcareous, , 
	Concretions; Field pH 9 (Raupach); 
	B2k	0.4 - 0.5 m	Light brown (7.5YR6/4-Moist); , 5YR46; Sandy clay loam; Massive grade of structure; Dry; 
	Strong consistence; Common (10 - 20 %), Calcareous, , Concretions; Field pH 9 (Raupach); 
	Gradual change to - 
	2B2	0.5 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moderate grade of structure, Subangular blocky; 
	Dry; Strong consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	2B2	0.6 - 0.8 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moderate grade of structure, Subangular blocky; 
	Dry; Strong consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	2B2k	0.8 - 1 m	Reddish yellow (7.5YR6/6-Moist); , 5YR44; Sandy clay; Massive grade of structure; Weak 
	grade of structure, Angular blocky; Dry; Strong consistence; 0-2%, cobbly, 60-200mm, Schist, 
	coarse fragments; Very many (50 - 100 %), Calcareous, , Concretions; Field pH 9 (Raupach); 
	2B2k	1 - 1.2 m	Reddish yellow (7.5YR6/6-Moist); ; Clay loam; Massive grade of structure; Dry; Very firm 
	consistence; 2-10%, coarse gravelly, 20-60mm, Schist, coarse fragments; Many (20 - 50 %), 
	Calcareous, , Concretions; Field pH 9 (Raupach); Diffuse change to - 
	3C	1.2 - 1.4 m	Reddish yellow (7.5YR7/6-Moist); , 7.5YR40; Sandy loam; Massive grade of structure; Moist; 
	Loose consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 9 (Raupach); 
	3C	1.4 - 1.6 m	Yellowish brown (10YR5/4-Moist); , 7.5YR40; Sandy loam; Massive grade of structure; Strong 
	consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 9 (Raupach); Diffuse 
	change to - 

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	3R	1.6 - 1.8 m	Rock 
	Morphological Notes
	B2	Transition from clay to carbonate.
	B2k	Some clay pockets in carbonate matrix.
	2B2	Carbonate film on pedological accumulation.
	2B2k	Zone of maximum carbonate accumulation.
	3C	Weathering schist inclusion.
	3R	Dark grey weathering schist.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.9A	0.07A	1.5K	0.36	0.91	0.12	7J	1.71
	0.1 - 0.18
	0.18 - 0.3	8.7A	0.31A	3.5K	4.8	1.4	4.2	15J	28.00
	0.3 - 0.4
	0.4 - 0.5	9.8A	0.65A	4.4K	4.8	1.3	4.1	17J	24.12
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1	9.7A	0.77A	4.5K	5.6	1.5	5.1	19J	26.84
	1 - 1.2
	1.2 - 1.4	9.8A	0.54A	3.2K	2.1	0.57	2.2	8J	27.50
	1.4 - 1.6
	1.6 - 1.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	<0.1C	3I	68	3	9
	0.1 - 0.18
	0.18 - 0.3	<0.1C	4I	51	4	31
	0.3 - 0.4
	0.4 - 0.5	12C	6I	48	6	25
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1	22C	3I	38	3	28
	1 - 1.2
	1.2 - 1.4	19C	3I	63	3	14
	1.4 - 1.6
	1.6 - 1.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.18
	0.18 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2
	1.2 - 1.4
	1.4 - 1.6
	1.6 - 1.8

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded