Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	21/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6112400 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	330110  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.33
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Reddish brown (5YR4/3-Moist); ; Loamy sand; Massive grade of structure; Dry; Very weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Field pH 6.5 
	(Raupach); Clear change to - 
	A2	0.1 - 0.2 m	Dark reddish grey (5YR4/2-Moist); , 5YR73; Loamy sand; Massive grade of structure; Dry; Very
	 firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Field pH 
	6.5 (Raupach); Sharp change to - 
	AB	0.2 - 0.3 m	Red (2.5YR4/6-Moist); ; Sandy clay; , Angular blocky; , Columnar; Dry; Strong consistence; Field
	 pH 7 (Raupach); 
	B2t	0.3 - 0.4 m	Red (2.5YR4/6-Moist); ; Sandy clay; , Angular blocky; Moderate grade of structure, 50-100 mm, 
	Prismatic; Dry; Strong consistence; Common (10 - 20 %), Calcareous, , ; Field pH 7.5 
	(Raupach); Clear change to - 
	B2tk	0.4 - 0.5 m	Reddish yellow (7.5YR6/6-Moist); , 5YR78; Clay loam; Massive grade of structure; Weak grade 
	of structure, Platy; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, 
	coarse fragments; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 8.5 
	(Raupach); 
	C1k	0.5 - 0.6 m	Reddish yellow (7.5YR6/6-Moist); , 5YR78; Sandy clay loam; Massive grade of structure; Weak 
	grade of structure, Platy; Dry; Very firm consistence; Common (10 - 20 %), Calcareous, , ; Field 
	pH 9 (Raupach); 
	C1k	0.6 - 0.7 m	Reddish yellow (7.5YR6/6-Moist); , 5YR78; Sandy clay loam; Massive grade of structure; Weak 
	grade of structure, Platy; Dry; Very firm consistence; 0-2%, medium gravelly, 6-20mm, Schist, 
	coarse fragments; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	C2k	0.7 - 0.8 m	Reddish yellow (7.5YR6/6-Moist); , 10YR52; Clay loam; Massive grade of structure; , Platy; 
	Very firm consistence; 20-50%, medium gravelly, 6-20mm, Schist, coarse fragments; Many (20 
	- 50 %), Calcareous, , ; Field pH 9 (Raupach); 
	C2k	0.8 - 0.9 m	Reddish yellow (7.5YR6/6-Moist); , 10YR52, 0-2% ; Silty loam; Massive grade of structure; , 
	Platy; Very firm consistence; Many (20 - 50 %), Calcareous, , Concretions; Field pH 9 
	(Raupach); Gradual change to - 
	2R	0.9 - 1.2 m	Rock 
	Morphological Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	A2	This horizon tongues into clay below causing irregularities in the boundary at 10cm.
	AB	Very sandy at top.  Many sand filled burrows.  SC texture is uncertain.
	B2t	 SC texture is uncertain.
	B2tk	Mainly semi-hard lime.  Some pockets of clay from above persist.
	C2k	60% semi-hard lime.  40% weathering schist.
	C2k	50/50 % weathering schist and carbonate matrix.
	2R	Mainly weathering schist.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.5A	0.06A	1.8K	0.6	0.84	0.03	5J	0.60
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4	8A	0.06A	13.3K	5.4	1.2	0.65	22J	2.95
	0.4 - 0.5	8.9A	0.11A	18.6K	6.4	1.3	0.83	27J	3.07
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8	9.1A	0.12A	16.8K	7	0.89	0.65	20J	3.25
	0.8 - 0.9
	0.9 - 1.2
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	<0.1C	8I	47	8	1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4	<0.1C	2I	25	2	32
	0.4 - 0.5	19C	5I	17	5	32
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8	20C	11I	17	11	20
	0.8 - 0.9
	0.9 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1.2

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded