Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	21/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6110720 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	326790  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gc1.11
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark brown (7.5YR3/2-Moist); ; Sandy clay loam; Weak grade of structure; Very weak 
	consistence; Few (2 - 10 %), Calcareous, , ; Field pH 8 (Raupach); Clear change to - 
	0.08 - 0.15 m	Reddish brown (5YR4/4-Moist); ; Sandy clay; Moderate grade of structure, Angular blocky; 
	Very firm consistence; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few (2
	 - 10 %), Calcareous, , ; Field pH 8.5 (Raupach); Gradual change to - 
	0.15 - 0.3 m	Yellowish red (5YR5/6-Moist); , 10YR82; Sandy clay; Massive grade of structure; Firm 
	consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 (Raupach); 
	0.3 - 0.41 m	Reddish yellow (7.5YR6/6-Moist); ; Clay loam; Massive grade of structure; Firm consistence; 
	Common (10 - 20 %), Calcareous, , Nodules; Field pH 9 (Raupach); Clear change to - 
	0.41 - 0.55 m	Reddish yellow (7.5YR6/6-Moist); , 10YR82; Clay loam; , Platy; Firm consistence; Common (10 - 
	20 %), Calcareous, , Nodules; Field pH 9 (Raupach); 
	0.55 - 0.66 m	Pink (7.5YR7/4-Moist); , 5YR56; Clay loam; , Platy; Firm consistence; Many (20 - 50 %), 
	Calcareous, , Concretions; Field pH 9 (Raupach); Clear change to - 
	0.66 - 0.8 m	Pink (7.5YR7/4-Moist); , 5YR46; Sandy clay loam; Massive grade of structure; Firm consistence;
	 Common (10 - 20 %), Calcareous, , Concretions; Field pH 9 (Raupach); 
	0.8 - 1 m	Yellowish red (5YR4/6-Moist); , 10YR53; , 10YR84; Sandy clay; Massive grade of structure; 
	Very firm consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Many 
	(20 - 50 %), Calcareous, , ; Field pH 9 (Raupach); 
	1 - 1.16 m	Yellowish red (5YR4/6-Moist); , 10YR53; , 10YR84; Sandy clay; Massive grade of structure, 
	Prismatic; Moderate grade of structure, Angular blocky; Very firm consistence; 0-2%, fine 
	gravelly, 2-6mm, subangular, Quartz, coarse fragments; Many (20 - 50 %), Calcareous, , ; Field 
	pH 9 (Raupach); 
	1.16 - 1.3 m	Yellowish red (5YR4/6-Moist); , 10YR53; , 10YR84; Sandy clay; , Angular blocky; Strong grade 
	of structure, Prismatic; Very firm consistence; Many (20 - 50 %), Calcareous, , ; Field pH 9 
	(Raupach); 
	1.3 - 1.5 m	Brown (7.5YR5/4-Moist); , 10YR54; Sandy clay; , Angular blocky; Strong grade of structure, 
	Prismatic; Very strong consistence; 2-10%, medium gravelly, 6-20mm, subangular, Quartz, 
	coarse fragments; Very few (0 - 2 %), Calcareous, , ; Field pH 9 (Raupach); Gradual change to

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	1.5 - 1.7 m	Brown (7.5YR5/4-Moist); , 10YR54; Sandy clay; , Angular blocky; Strong grade of structure, 
	Prismatic; Very strong consistence; 2-10%, medium gravelly, 6-20mm, subangular, Quartz, 
	coarse fragments; Field pH 8.5 (Raupach); Gradual change to - 
	1.7 - 2 m	Brown (7.5YR5/4-Moist); , 10YR54; Sandy clay; Strong consistence; 2-10%, medium gravelly, 
	6-20mm, subangular, Quartz, coarse fragments; Field pH 7.5 (Raupach); Clear change to - 
	2 - 2.3 m	Brown (7.5YR5/4-Moist); , 10YR54; Sandy clay; Strong consistence; Field pH 6.5 (Raupach); 
	Morphological Notes
	Highly vesicular.  SC texture is uncertain.
	Highly porous.  Carbonate nodules.  SC texture is uncertain.
	Highly porous.  Carbonate nodules.
	Increased amounts of Blanchetown clay in carbonate matrix, clay and lime more 
	intimately mixed.
	SC texture is uncertain.
	SC texture is uncertain.
	Mainly Blanchetown clay with occassional lime pockets persisting.  SC texture is 
	Mainly Blanchetown clay with occassional lime pockets persisting.  SC texture is 
	SC texture is uncertain.
	SC texture is uncertain.
	SC texture is uncertain.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.6A	0.18A	16.4K	3.6	2.9	0.77	27J	2.85
	0.08 - 0.15	8.5A	0.1A	18.7K	3.2	1.9	0.42	28J	1.50
	0.15 - 0.3	8.9A	0.11A	9K	6.9	1.5	4.1	23J	17.83
	0.3 - 0.41
	0.41 - 0.55	9.9A	0.4A	5.4K	6.3	1.8	8.4	22J	38.18
	0.55 - 0.66
	0.66 - 0.8
	0.8 - 1	10A	1.02A	5.4K	6.3	1.8	8.5	22J	38.64
	1 - 1.16
	1.16 - 1.3
	1.3 - 1.5
	1.5 - 1.7	8.5A	1.3A	0.53K	7.9	2	10.4	25J	41.60
	1.7 - 2
	2 - 2.3
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	4.4C	7I	40	7	23
	0.08 - 0.15	2.8C	4I	46	4	28
	0.15 - 0.3	18C	2I	36	2	24
	0.3 - 0.41
	0.41 - 0.55	51C	3I	20	3	16
	0.55 - 0.66
	0.66 - 0.8
	0.8 - 1	55C	1I	14	1	22
	1 - 1.16
	1.16 - 1.3
	1.3 - 1.5
	1.5 - 1.7	<0.1C	2I	36	2	38
	1.7 - 2
	2 - 2.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.3
	0.3 - 0.41
	0.41 - 0.55
	0.55 - 0.66
	0.66 - 0.8
	0.8 - 1
	1 - 1.16
	1.16 - 1.3
	1.3 - 1.5
	1.5 - 1.7
	1.7 - 2
	2 - 2.3

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded