Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	21/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6108020 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	330120  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug3.2
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (5YR4/1-Moist); ; Sandy clay; Massive grade of structure; Loose consistence; Few 
	(2 - 10 %), Calcareous, , ; Field pH 9.5 (Raupach); Clear change to - 
	A2	0.1 - 0.31 m	Light grey (5Y7/2-Moist); , 10YR42; Sandy clay; Weak grade of structure, Prismatic; Very weak
	 consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Many (20 - 
	50 %), Calcareous, , ; Field pH 9.5 (Raupach); Gradual change to - 
	C1	0.31 - 0.5 m	Greyish brown (10YR5/2-Moist); , 10YR66, 0-2% ; Sandy clay; Strong grade of structure, 50-
	100 mm, Angular blocky; Strong consistence; Common (10 - 20 %), Calcareous, , ; Field pH 9 
	(Raupach); Diffuse change to - 
	C2	0.5 - 0.9 m	Brownish yellow (10YR6/6-Moist); , 10YR52; Sandy clay; Strong grade of structure, 50-100 
	mm, Angular blocky; Strong consistence; Few (2 - 10 %), Calcareous, , ; Field pH 8.5 
	(Raupach); Diffuse change to - 
	C3	0.9 - 2 m	Yellowish brown (10YR5/4-Moist); , 2.5Y62; Sandy clay; 100-200 mm, Angular blocky; Very 
	firm consistence; Few (2 - 10 %), Calcareous, , ; Field pH 9 (Raupach); 
	Morphological Notes
	A1	SC texture is uncertain.
	A2	SC texture is uncertain.  Sporadic bleach.
	C1	SC texture is uncertain.
	C2	SC texture is uncertain.  Strongly cracked.
	C3	SC texture is uncertain.  Strongly cracked.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.7A	0.14A	16.3K	4	1.9	0.44	23J	1.91
	0.1 - 0.31	8.8A	0.14A
	0.31 - 0.5	9.1A	0.37A	11.1K	6.4	1	2.7	21J	12.86
	0.5 - 0.9	9.1A	0.82A	7.5K	6.5	0.95	4.3	19J	22.63
	0.9 - 2	9.1A	0.73A	5.8K	6.7	0.99	6.9	19J	36.32
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	8.2C	4I	28	4	28
	0.1 - 0.31
	0.31 - 0.5	13C	2I	16	2	40
	0.5 - 0.9	5.2C	2I	21	2	36
	0.9 - 2	4C	2I	20	2	41
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.31
	0.31 - 0.5
	0.5 - 0.9
	0.9 - 2

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded