Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1190	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	21/11/75	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	6122570 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	339180  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.08 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Firm 
	consistence; Sharp, Broken change to - 
	0.08 - 0.17 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; 50-100 mm, Prismatic; Strong consistence; 0-
	2%, coarse fragments; Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.17 - 0.45 m	Yellowish red (5YR4/6-Moist); ; Fine sandy clay; Massive grade of structure; Strong 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.45 - 0.9 m	Yellowish red (5YR5/6-Moist); , 10YR42; Clay loam; Massive grade of structure; Strong 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.9 - 1.7 m	Dark red (2.5YR3/6-Moist); ; Clayey sand; 50-100 mm, Angular blocky; Strong consistence; 
	Very few (0 - 2 %), Calcareous, , ; Diffuse change to - 
	1.7 - 1.8 m	; Sandy loam; Weak grade of structure, 50-100 mm; Firm consistence; Very few (0 - 2 %), 
	Calcareous, , ; 
	Morphological Notes
	Surface grit and gravel present.
	Texture FSC is uncertain.
	Structure: weak 50-100mm clod.
	Observation Notes
	Site Notes

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1190	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.4A	0.13A	9.7K	1.9	1.2	0.17	13J	1.31
	0.08 - 0.17	8.8A	0.1A	11K	3.5	0.77	0.3	16J	1.88
	0.17 - 0.45
	0.45 - 0.9	9.9A	0.46A	2.6K	6.2	0.72	4	12J	33.33
	0.9 - 1.2
	1.2 - 1.8	9.8A	0.33A	0.92K	1.9	0.36	2.1	5J	42.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	0.1C	7I	46	7	16
	0.08 - 0.17	3.4C	6I	42	6	21
	0.17 - 0.45
	0.45 - 0.9	6.5C	8I	37	8	22
	0.9 - 1.2
	1.2 - 1.8	0.3C	2I	48	2	12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.17
	0.17 - 0.45
	0.45 - 0.9
	0.9 - 1.2
	1.2 - 1.8

	Project Name:	Soils of the MonartoTown Site
	Project Code:	Monarto	Site ID:	A1190	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded