Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BIL	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	15/04/97	Elevation:	91 metres
	Map Ref.:	Sheet No. : 7827   1:100000	Rainfall:	No Data
	Northing/Long.:	6078703 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	312859  Datum: AGD66	Drainage:	Very poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.9 m deep,Slightly porous, 
	Colluvium 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Backplain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Subnatric Grey Sodosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44, 2-10% , 0-5mm, Distinct; , 10YR51, 2-10% , 0-
	5mm, Distinct; Clay loam; Moderate grade of structure, 20-50 mm, Subangular blocky; Massive 
	grade of structure; Rough-ped fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very 
	fine (0.075-1mm) macropores, Wet; Very plastic; Normal plasticity; Very sticky; Field pH 6 
	(Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	A12	0.1 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44, 10-20% , 0-5mm, Distinct; , 10YR51, 10-20% , 
	0-5mm, Distinct; Clay loam; Weak grade of structure, 10-20 mm, Subangular blocky; Massive 
	grade of structure; Rough-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Wet; Moderately plastic; Normal plasticity; Very sticky; Field pH 6 (Raupach); 
	Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B21	0.3 - 0.5 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR44, 2-10% , 0-5mm, Distinct; Light medium clay; 
	Moderate grade of structure, 2-5 mm, Subangular blocky; Massive grade of structure; Smooth-
	ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very plastic; 
	Normal plasticity; Very sticky; Common cutans, 10-50% of ped faces or walls coated, distinct; 
	Field pH 6 (Raupach); Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	B22	0.5 - 0.7 m	Dark grey (10YR4/1-Moist); , 7.5YR44, 2-10% , 0-5mm, Faint; , 10YR51, 2-10% , 0-5mm, Faint; 
	Medium clay; Moderate grade of structure, 5-10 mm, Lenticular; Massive grade of structure; 
	Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very 
	plastic; Normal plasticity; Very sticky; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Concretions; Field pH 10 (Raupach); 
	Gradual, Smooth change to - 
	Bk	0.7 - 0.9 m	Dark greyish brown (2.5Y4/2-Moist); , 0-0% ; Medium clay; Moderate grade of structure, 5-10 
	mm, Lenticular; Massive grade of structure; Smooth-ped fabric; Few (<1 per 100mm2) Very fine
	 (0.075-1mm) macropores, Moist; Very plastic; Normal plasticity; Very sticky; Many cutans, 
	>50% of ped faces or walls coated, distinct; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Field pH 10 (Raupach); Gradual, Smooth change to - 
	BC	0.9 - 1.3 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y56, 10-20% , 5-15mm, Distinct; Medium clay; 
	Massive grade of structure; Rough-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moderately moist; Very plastic; Normal plasticity; Very sticky; Many cutans, >50% 
	of ped faces or walls coated, distinct; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Concretions; Field pH 10 (Raupach); Gradual, Smooth change to - 

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BIL	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	C	1.3 - 1.5 m	Light grey (2.5Y7/1-Moist); , 10YR58, 20-50% , 5-15mm, Distinct; Light medium clay; Massive 
	grade of structure; Rough-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moderately moist; Very plastic; Normal plasticity; Very sticky; Few (2 - 10 %), 
	Ferruginous, Fine (0 - 2 mm), Concretions; Field pH 10 (Raupach); 
	Morphological Notes
	Observation Notes
	Vertic, Sub-natric, Grey Sodosol, medium, non-gravelly, clay loamy, clayey, deep
	Site Notes
	DENILIQUIN, BILLINUDGEL Photos surface 83/12, profile 83/13, rice soil with alot of organic matter, 2yr old, Vertic, Sub-natric, 
	Grey Sodosol, medium, non-gravelly, clay loamy, clayey, deep

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BIL	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	BIL	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile