Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	KAR	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	13/03/97	Elevation:	95 metres
	Map Ref.:	Sheet No. : 7927   1:100000	Rainfall:	No Data
	Northing/Long.:	6077833 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	336203  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.55 m deep,Porous, Sand 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Prior stream	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mesotrophic Red Kandosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Sandy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus melliodora, Casuarina leuhmannii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.2 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Many (>5 per 
	100mm2) Fine (1-2mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Non-plastic; Normal 
	plasticity; Non-sticky; 0-2%, medium gravelly, 6-20mm, rounded, dispersed, Quartz, coarse 
	fragments; 0-2%, medium gravelly, 6-20mm, dispersed, Quartz, coarse fragments; 0-2%, 
	medium gravelly, 6-20mm, rounded, dispersed, Quartz, coarse fragments; Field pH 6.5 
	(Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	A12	0.2 - 0.4 m	Yellowish red (5YR4/8-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Moist; Non-plastic; Normal plasticity; Non-sticky; 0-2%, medium 
	gravelly, 6-20mm, rounded, dispersed, Quartz, coarse fragments; Field pH 6.5 (Raupach); 
	Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	B2	0.4 - 0.55 m	Yellowish red (5YR5/8-Moist); , 0-0% ; Coarse sandy clay loam; Single grain grade of structure;
	 Earthy fabric; Moist; Slightly plastic; Normal plasticity; Moderately sticky; 0-2%, medium gravelly,
	 6-20mm, rounded, dispersed, Quartz, coarse fragments; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Field pH 6.5 (Raupach); Common, fine (1-2mm) roots; Gradual, 
	Smooth change to - 
	C1	0.55 - 1 m	Strong brown (7.5YR4/6-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Moist; Non-plastic; Normal plasticity; Non-sticky; 0-2%, medium 
	gravelly, 6-20mm, rounded, dispersed, Quartz, coarse fragments; Field pH 7 (Raupach); Few, 
	fine (1-2mm) roots; Gradual, Smooth change to - 
	C2	1 - 1.1 m	Dark yellowish brown (10YR4/4-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; 
	Sandy (grains prominent) fabric; Wet; Non-plastic; Normal plasticity; Non-sticky; 0-2%, medium 
	gravelly, 6-20mm, rounded, dispersed, Quartz, coarse fragments; Field pH 7.5 (Raupach); Few,
	 fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	DENILIQUIN, KARAWATHA;  Photo surface 29,30,18 and profile 17. Planted 1995. 2m spacing Kandosol, red, mesotrophic, 

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	KAR	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	KAR	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	KAR	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile