Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MCIN	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	27/02/97	Elevation:	70 metres
	Map Ref.:	Sheet No. : 7022   1:100000	Rainfall:	No Data
	Northing/Long.:	5843155 AMG zone: 54	Runoff:	No runoff
	Easting/Lat.:	460522  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Qpcp	Substrate Material:	Auger boring, 0.7 m deep,Slightly porous, 
	Lacustrine Sediment 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Chenier plain
	3%
	Morph. Type:	Flat	Relief:	2 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Petroferric Brown Chromosol Thick Non-gravelly 	Principal Profile Form:	N/A
	Sandy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - Eucalyptus globulus
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, 10-20 
	mm, Subangular blocky; Rough-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, 
	Dry; Non-plastic; Normal plasticity; Non-sticky; Field pH 5 (Raupach); Many, fine (1-2mm) roots; 
	Clear, Smooth change to - 
	A12	0.1 - 0.5 m	Greyish brown (10YR5/2-Moist); , 0-0% ; Loamy sand; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Non-
	plastic; Normal plasticity; Non-sticky; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B1	0.5 - 0.6 m	Brown (10YR5/3-Moist); , 7.5YR56, 0-2% , 5-15mm, Faint; Clayey sand; Weak grade of 
	structure, 10-20 mm, Subangular blocky; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Non-plastic; Normal plasticity; Slightly sticky; 0-2%, medium gravelly, 6-20mm, 
	rounded, dispersed, Ferricrete, coarse fragments; 0-2%, medium gravelly, 6-20mm, rounded, 
	dispersed, Substrate material, coarse fragments; Field pH 6 (Raupach); Few, fine (1-2mm) 
	roots; Clear, Smooth change to - 
	B2	0.6 - 0.7 m	Yellowish brown (10YR5/4-Moist); , 7.5YR56, 0-2% , 5-15mm, Faint; Sandy clay loam; Massive 
	grade of structure; Earthy fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Slightly plastic; Normal plasticity; Moderately sticky; 10-20%, medium gravelly, 
	6-20mm, rounded, dispersed, Ferricrete, coarse fragments; 10-20%, medium gravelly, 6-20mm, 
	rounded, dispersed, Ferricrete, coarse fragments; Few cutans, <10% of ped faces or walls 
	coated, distinct; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Manganiferous pan, Weakly cemented, 
	Discontinuous, Platy; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Sharp, Smooth change to - 
	D1	0.7 - 0.9 m	Brown (10YR5/3-Moist); , 0-0% ; Sandy medium clay; Massive grade of structure; Rough-ped 
	fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Very plastic; 
	Normal plasticity; Moderately sticky; Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Many (20 - 50 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 6 
	(Raupach); Few, fine (1-2mm) roots; Abrupt, Smooth change to - 

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MCIN	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	D2	0.9 - 1.4 m	Light brownish grey (2.5Y6/2-Moist); , 2.5YR48, 10-20% , 5-15mm, Distinct; , 7.5YR58, 10-20% 
	, 5-15mm, Distinct; Medium clay; Massive grade of structure; Rough-ped fabric; Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Very plastic; Normal plasticity; 
	Moderately sticky; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Abrupt, Smooth change to - 
	D3	1.4 - 1.9 m	Light grey (2.5Y7/0-Moist); , 2.5YR48, 20-50% , 15-30mm, Distinct; Medium heavy clay; Massive
	 grade of structure; Rough-ped fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Very plastic; Normal plasticity; Moderately sticky; Field pH 6 (Raupach); Few, 
	fine (1-2mm) roots; Abrupt, Smooth change to - 
	D4	1.9 - 2 m	Light grey (2.5Y7/2-Moist); , 10YR58, 2-10% , 15-30mm, Distinct; , 2.5YR36, 2-10% , 15-30mm, 
	Distinct; Medium heavy clay; Massive grade of structure; Rough-ped fabric; Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Very plastic; Normal plasticity; 
	Moderately sticky; Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	MT MUIR SAND, Mottled, Petroferric?, Brown chromosol, thick, non-gravelly, sandy, clay loamy, moderate
	Site Notes
	MT EDWARD SE SOUTH AUSTRALIA, "red gum" type site which should be doing better, MT MUIR SAND, Mottled, Petroferric?, 
	Brown chromosol, thick, non-gravelly, sandy, clay loamy, moderate

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MCIN	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MCIN	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile