Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MEA3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	18/02/97	Elevation:	410 metres
	Map Ref.:	Sheet No. : 6627-1   1:100000	Rainfall:	No Data
	Northing/Long.:	6105558 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	297684  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.7 m deep,Slightly porous, 
	Clay 
	Land Form
	Rel/Slope Class: 	Rolling hills 90-300m 10-32%	Pattern Type:	Hills
	Morph. Type:	Flat	Relief:	60 metres
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic-Mottled Mesotrophic Grey Chromosol Medium Non-	Principal Profile Form:	N/A
	gravelly Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.2 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Silty clay loam; Strong grade of structure, 2-5 mm, 
	Subangular blocky; Moderate grade of structure, 2-5 mm, Subangular blocky; Weak grade of 
	structure, 5-10 mm, Subangular blocky; Rough-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) 
	macropores, Moderately moist; Slightly plastic; Normal plasticity; Moderately sticky; Field pH 6 
	(Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B2g	0.2 - 0.5 m	Dark greyish brown (10YR4/2-Moist); , 10YR41, 10-20% , 5-15mm, Faint; Silty light clay; 
	Moderate grade of structure, 2-5 mm, Subangular blocky; Rough-ped fabric; Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Moderately plastic; Normal plasticity; 
	Moderately sticky; Common cutans, 10-50% of ped faces or walls coated, distinct; Field pH 6 
	(Raupach); Few, fine (1-2mm) roots; Clear, Smooth change to - 
	B2	0.5 - 0.7 m	Yellowish brown (10YR5/6-Moist); , 2.5YR48, 0-2% , 0-5mm, Distinct; Medium clay; Weak grade
	 of structure, 5-10 mm, Subangular blocky; Rough-ped fabric; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Moderately moist; Very plastic; Normal plasticity; Moderately sticky; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; Field pH 6.5 (Raupach); Few, fine (1-
	2mm) roots; Clear, Smooth change to - 
	BC	0.7 - 1 m	Yellowish brown (10YR5/4-Moist); , 2.5YR46, 0-2% , 15-30mm, Distinct; Light clay; Weak grade
	 of structure, 10-20 mm, Subangular blocky; Earthy fabric; Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Moderately moist; Very plastic; Normal plasticity; Moderately sticky; Few cutans, 
	<10% of ped faces or walls coated, distinct; Field pH 6.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Litter layer, no ground cover. 8yr old grandis plantation.
	Site Notes
	MEADOWS, SOUTHERN MT LOFTY RANGES, Handiside property. valley flat.Melanic-mottled, Mesotrophic, Grey, Chromosol; 
	non-gravelly, clay loamy, clayey, moderate

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MEA3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	MEA3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile