Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	OAK1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	16/04/97	Elevation:	94 metres
	Map Ref.:	Sheet No. : 7826   1:100000	Rainfall:	No Data
	Northing/Long.:	6059041 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	317025  Datum: AGD66	Drainage:	Very poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.8 m deep,Slightly porous, 
	Colluvium 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Swamp	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Crusty Grey Vertosol Not recorded Non-	Principal Profile Form:	N/A
	gravelly Very fine Very fine Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 10YR51, 2-10% , 0-5mm, Distinct; Medium heavy clay; 
	Moderate grade of structure, 2-5 mm, Polyhedral; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Medium, (5 - 10) mm crack; Common (1-5 per 100mm2) 
	Fine (1-2mm) macropores, Moderately moist; Very plastic; Normal plasticity; Moderately sticky; 
	Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B1g	0.1 - 0.2 m	Olive grey (5Y4/2-Moist); , 7.5YR44, 2-10% , 0-5mm, Distinct; Heavy clay; Moderate grade of 
	structure, 2-5 mm, Lenticular; Massive grade of structure; Smooth-ped fabric; Fine, (0 - 5) mm 
	crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Wet; Very plastic; Normal 
	plasticity; Moderately sticky; Common cutans, 10-50% of ped faces or walls coated, distinct; 
	Field pH 6.5 (Raupach); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B2g	0.2 - 0.5 m	Olive grey (5Y4/2-Moist); , 7.5YR44, 2-10% , 0-5mm, Distinct; Heavy clay; Moderate grade of 
	structure, 2-5 mm, Lenticular; Massive grade of structure; Smooth-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Wet; Very plastic; Normal plasticity; Very sticky; 
	Common cutans, 10-50% of ped faces or walls coated, distinct; Field pH 7.5 (Raupach); 
	Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	BC	0.5 - 0.9 m	Dark greyish brown (2.5Y4/2-Moist); , 0-0% ; Medium heavy clay; Moderate grade of structure, 
	5-10 mm, Lenticular; Massive grade of structure; Smooth-ped fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Moist; Very plastic; Normal plasticity; Very sticky; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; Very few (0 - 2 %), Calcareous, Medium
	 (2 -6 mm), Soft segregations; Field pH 10 (Raupach); Clear, Smooth change to - 
	D	0.9 - 1.5 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR56, 10-20% , 5-15mm, Distinct; Medium clay; 
	Moderate grade of structure, 10-20 mm, Lenticular; Massive grade of structure; Rough-ped 
	fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very plastic; Normal 
	plasticity; Moderately sticky; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Concretions; Few
	 (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Soft segregations; Very few (0 - 2 %), 
	Calcareous, Medium (2 -6 mm), Soft segregations; Very few (0 - 2 %), Gypseous, Medium (2 -6
	 mm), Crystals; Field pH 10 (Raupach); 
	Morphological Notes
	Observation Notes
	Epihypersodic, Crusty, Grey vertosol, non-gravelly, very fine, very fine, moderate, very poor drainage

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	OAK1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Notes
	OAKBANK, DENILIQUIN, Photo surface 84/6, profile 84/5, Epihypersodic, Crusty, Grey vertosol, non-gravelly, very fine, very 
	fine, moderate. poor growth on block, poor drainage. E. camaldulensis remnant vegetation

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	OAK1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	OAK1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile