Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	STR1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	26/02/97	Elevation:	50 metres
	Map Ref.:	Sheet No. : 7122   1:10000	Rainfall:	No Data
	Northing/Long.:	5826996 AMG zone: 54	Runoff:	No runoff
	Easting/Lat.:	514455  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 2 m deep,Slightly porous, 
	Eolian sand 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Chenier plain
	3%
	Morph. Type:	Flat	Relief:	3 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Parapanic Humosequic Semiaquic Podosol Medium Non-	Principal Profile Form:	N/A
	gravelly Sandy Sandy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.2 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Non-
	plastic; Normal plasticity; Non-sticky; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	A12	0.2 - 0.5 m	Grey (10YR5/1-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Non-plastic; Normal plasticity; 
	Non-sticky; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Chert, coarse fragments; Field pH 6 
	(Raupach); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	A2e	0.5 - 0.8 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Non-plastic; 
	Normal plasticity; Non-sticky; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Chert, coarse 
	fragments; Field pH 6.5 (Raupach); Few, fine (1-2mm) roots; Sharp, Irregular change to - 
	Bhs	0.8 - 1 m	Brown (7.5YR5/4-Moist); , 10YR56, 10-20% , 5-15mm, Distinct; , 10YR81, 10-20% , 5-15mm, 
	Distinct; Sand; Massive grade of structure; Sandy (grains prominent) fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Normal plasticity; Non-sticky; 
	10-20%, coarse gravelly, 20-60mm, rounded, dispersed, Conglomerate, coarse fragments; 
	Many (20 - 50 %), Ferruginous-organic, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (Raupach); 
	Sharp, Irregular change to - 
	Bhsm	1 - 1.1 m	Brown (7.5YR5/4-Moist); , 0-0% ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Normal 
	plasticity; Non-sticky; 50-90%, coarse gravelly, 20-60mm, rounded, dispersed, Conglomerate, 
	coarse fragments; Very many (50 - 100 %), Ferruginous-organic, Coarse (6 - 20 mm), Nodules;
	 Ortstein, Strongly cemented, Continuous, Massive; Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Nangawary Sand; Parapanic, Humosequic, Semiaquic, Podosol, medium, non-gravelly, sandy, sandy, very deep
	Site Notes

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	STR1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	STRATHDOWNIE, SE SOUTH AUSTRALIA, Block 1, Treatment 6, Parapanic, Humosequic, Semiaquic, Podosol, medium, non-
	gravelly, sandy, sandy, very deep. PHOTO surface 76/3. better tree growth than Copes

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	STR1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	STR1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile