Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	UND	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/03/97	Elevation:	110 metres
	Map Ref.:	Sheet No. : 7925   1:100000	Rainfall:	No Data
	Northing/Long.:	5977874 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	341052  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.5 m deep,Slightly porous, 
	Colluvium 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Backplain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Poached
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Eucalyptus grandifolia, Eucalyptus camaldulensis, Eucalyptus 
	saligna
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Brown (7.5YR4/4-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 2-5 mm, Subangular 
	blocky; Rough-ped fabric; Medium, (5 - 10) mm crack; Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Wet; Moderately plastic; Normal plasticity; Moderately sticky; Field pH 7 (Raupach);
	 Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B21	0.15 - 0.2 m	Dark red (2.5YR3/6-Moist); , 0-0% ; Medium clay; Massive grade of structure; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Wet; Moderately plastic; Normal plasticity; Very 
	sticky; Field pH 7 (Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B22	0.2 - 0.5 m	Dark red (2.5YR3/6-Moist); , 0-0% ; Medium heavy clay; Massive grade of structure; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Wet; Moderately plastic; Normal plasticity; 
	Very sticky; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 7.5 (Raupach); 
	Few, fine (1-2mm) roots; Clear, Smooth change to - 
	C	0.5 - 1 m	Strong brown (7.5YR5/6-Moist); , 0-0% ; Medium clay; Massive grade of structure; Few (<1 per
	 100mm2) Very fine (0.075-1mm) macropores, Moist; Very plastic; Normal plasticity; Moderately 
	sticky; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9 (Raupach); Few, 
	fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Sodic, Mesotrophic, Brown Chromosol; medium, non-gravelly, clay loamy, clayey, moderate, similar to Timmering and 
	Tatura,irrigation turned off,
	Site Notes
	UNDERA, SHEPPARTON, Photo surface: 78/25, 79/1; similar to Tatura, irrigation turned off, Sodic, Mesotrophic, Brown 
	Chromosol; medium, non-gravelly, clay loamy, clayey, moderate, planted 1991, preliminary site for TFP, poor growth

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	UND	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	New Farm Forest
	Project Code:	NFF	Site ID:	UND	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile