Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP12	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Thompson, Jim	Locality:
	Date Desc.:	21/12/71	Elevation:	No Data
	Map Ref.:	Sheet No. : 7024   1:100000	Rainfall:	650
	Northing/Long.:	140.95	Runoff:	No Data
	Easting/Lat.:	-37.1333333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.23
	ASC Confidence:	Great Soil Group:	Siliceous sand
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; , 0-0% ; Loamy sand; Massive grade of structure; Very weak 
	consistence; 
	0.1 - 0.15 m	Brown (10YR5/3-Moist); , 0-0% ; , 0-0% ; Loamy sand; Massive grade of structure; Very weak 
	consistence; 
	0.15 - 0.2 m	Dark brown (10YR3/3-Moist); , 5YR48, 2-10% , Faint; , 2-10% , Faint; Light clay; Strong grade 
	of structure, 5-10 mm, Subangular blocky; Very strong consistence; 
	0.2 - 0.3 m	Very dark greyish brown (10YR3/2-Moist); , 5YR48, 10-20% , Faint; , 10-20% , Faint; Light clay;
	 Strong grade of structure, 5-10 mm, Subangular blocky; Very strong consistence; 
	0.3 - 0.4 m	Brown (10YR4/3-Moist); , 0-0% ; , 0-0% ; Light clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Very strong consistence; 
	0.4 - 0.5 m	Brown (10YR4/3-Moist); , 0-0% ; , 0-0% ; Light clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Very strong consistence; 
	0.5 - 0.6 m	Brown (10YR4/3-Moist); , 10YR82, 2-10% , Faint; , 2-10% , Faint; Light clay; Strong grade of 
	structure, 5-10 mm, Subangular blocky; Very strong consistence; Very few (0 - 2 %), 
	Calcareous, , Nodules; Soil matrix is Moderately calcareous; 
	0.6 - 0.7 m	Brown (10YR5/3-Moist); , 10YR83, 10-20% , Faint; , 5YR48, 10-20% , Faint; Light clay; Strong 
	grade of structure, 2-5 mm, Subangular blocky; Very strong consistence; 2-10%, Gravel, 
	coarse fragments; Common (10 - 20 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.7 - 0.8 m	White (2.5Y8/2-Moist); , 10YR43, 10-20% , Faint; , 10-20% , Faint; Light clay; Strong grade of 
	structure, 2-5 mm, Subangular blocky; Strong consistence; 2-10%, Gravel, coarse fragments; 
	Common (10 - 20 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.8 - 0.9 m	White (2.5Y8/2-Moist); , 10YR54, 10-20% , Faint; , 10-20% , Faint; Light clay; Strong grade of 
	structure, 2-5 mm, Subangular blocky; Strong consistence; 2-10%, Gravel, coarse fragments; 
	Common (10 - 20 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.9 - 0.95 m	White (2.5Y8/2-Moist); , 2.5Y42, 10-20% , Faint; , 10YR54, 10-20% , Faint; Light clay; Strong 
	grade of structure, 2-5 mm, Subangular blocky; Strong consistence; 2-10%, Gravel, coarse 
	fragments; Common (10 - 20 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	Morphological Notes

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP12	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Observation Notes
	SP71/P4; MORPHOLOGY FROM CORE NO.7; CHEMICAL DATA FROM BULK OF CORES 3-9;                                               
	Site Notes
	WRATIONBULLY

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP12	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8I	 0.11D
	0.1 - 0.15	6.3I	 0.09D
	0.15 - 0.2	6.3I	 0.129D
	0.2 - 0.3	6.8I	 0.36D
	0.3 - 0.4	7.5I	 0.62D
	0.4 - 0.5	8I	 0.77D
	0.5 - 0.6	8.9I	 0.92D
	0.6 - 0.7	9.1I	 0.94D
	0.7 - 0.8	9.2I	 0.89D
	0.8 - 0.9	9I	 1.11D
	0.9 - 0.95	8.9I	 1.27D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.139A	 18C	 61	 10	 9
	0.1 - 0.15	 0.04A	 12C	 43	 11	 34
	0.15 - 0.2	 0.055A
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6	 2.5C	 0.022A
	0.6 - 0.7	 17.2C
	0.7 - 0.8	 9.1C
	0.8 - 0.9	 3.6C
	0.9 - 0.95	 6.5C	 0.013A	 7C	 33	 11	 39
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 0.95

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP12	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction