Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Coppi, John	Locality:
	Date Desc.:	07/08/72	Elevation:	No Data
	Map Ref.:	Sheet No. : 6628   1:100000	Rainfall:	0
	Northing/Long.:	138.983333333333	Runoff:	No Data
	Easting/Lat.:	-34.7	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Metamorphic rock (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc
	ASC Confidence:	Great Soil Group:	Siliceous sand
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 0-2%, Gravel, coarse fragments; 
	0.1 - 0.2 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-
	2%, Gravel, coarse fragments; 
	0.2 - 0.3 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-
	2%, Gravel, coarse fragments; 
	0.3 - 0.4 m	Light grey (10YR7/1-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-
	2%, Gravel, coarse fragments; 
	0.4 - 0.5 m	Light grey (10YR7/2-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-
	2%, Gravel, coarse fragments; 
	0.5 - 0.6 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 0-2%, Gravel, coarse fragments; 
	0.6 - 0.7 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-2%,
	 Gravel, coarse fragments; 
	0.7 - 0.8 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 0-2%,
	 Gravel, coarse fragments; 
	0.8 - 0.9 m	Yellowish brown (10YR5/4-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 0-2%, Gravel, coarse fragments; 
	0.9 - 1 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 0-2%, Gravel, coarse fragments; 
	Morphological Notes
	Observation Notes
	ORIGINALLY SP72/P2; MORPHOLOGY FROM SINGLE CORE NO.6; CHEMICAL DATA FROM  BULK OF 8 CORES;                          
	    
	Site Notes
	WILLIAMSTOWN

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2I	 0.12D
	0.1 - 0.2	5.3I	 0D
	0.2 - 0.3	5.3I	 0D
	0.3 - 0.4	5.4I	 0D
	0.4 - 0.5	5.5I	 0.08D
	0.5 - 0.6	5.9I	 0.11D
	0.6 - 0.7	6.2I	 0.11D
	0.7 - 0.8	6.7I	 0.08D
	0.8 - 0.9	7I	 0.07D
	0.9 - 1	7.3I	 0.07D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.09A	 28C	 64	 1	 4
	0.1 - 0.2	 0.047A
	0.2 - 0.3	 0.025A
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6	 0.013A
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1	 0.005A	 28C	 64	 4	 4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded