Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP6	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Coppi, John	Locality:
	Date Desc.:	27/05/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7022   1:100000	Rainfall:	760
	Northing/Long.:	140.75	Runoff:	No Data
	Easting/Lat.:	-37.55	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	Confidence level not specified	soil
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Sand; Massive grade of structure; Very weak consistence; 0-2%, 
	Gravel, coarse fragments; 
	0.1 - 0.2 m	Brown (7.5YR4/2-Moist); ; Sand; Massive grade of structure; Very weak consistence; 0-2%, 
	Gravel, coarse fragments; 
	0.2 - 0.3 m	Brown (7.5YR4/2-Moist); ; Sand; Massive grade of structure; Very weak consistence; 0-2%, 
	Gravel, coarse fragments; 
	0.3 - 0.4 m	Brown (10YR5/3-Moist); ; Sand; Massive grade of structure; Very weak consistence; 0-2%, 
	Gravel, coarse fragments; 
	0.4 - 0.5 m	Brown (10YR5/3-Moist); ; Sand; Massive grade of structure; Very weak consistence; 0-2%, 
	Gravel, coarse fragments; 
	0.5 - 0.55 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; Strong grade of structure, 5-10 mm; Very
	 strong consistence; 0-2%, Gravel, coarse fragments; 
	0.55 - 0.6 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48, 10-20% , Distinct; , 10-20% , Distinct; Heavy 
	clay; Strong grade of structure, 5-10 mm; Very strong consistence; 0-2%, Gravel, coarse 
	0.6 - 0.7 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48, 10-20% , Distinct; , 10-20% , Distinct; Heavy 
	clay; Strong grade of structure, 5-10 mm; Very strong consistence; 0-2%, Gravel, coarse 
	0.7 - 0.8 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48, 10-20% , Distinct; , 10-20% , Distinct; Heavy 
	clay; Strong grade of structure, 5-10 mm; Very strong consistence; 0-2%, Gravel, coarse 
	0.8 - 0.9 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48, 10-20% , Distinct; , 10-20% , Distinct; Heavy 
	clay; Strong grade of structure, 5-10 mm; Very strong consistence; 0-2%, Gravel, coarse 
	0.9 - 1 m	Yellowish brown (10YR5/4-Moist); , 2.5YR48, 10-20% , Distinct; , 10-20% , Distinct; Heavy 
	clay; Strong grade of structure, 5-10 mm; Very strong consistence; 
	Morphological Notes
	Observation Notes
	SP70/P9; CHEMICAL DATA IS FROM BULK OF 8 CORES;                                                                         
	Site Notes

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP6	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	KALANGADOO

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP6	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7I	 0.53D
	0.1 - 0.2	5.6I	 0.16D
	0.2 - 0.3	5.9I	 0.08D
	0.3 - 0.4	6.4I	 0.08D
	0.4 - 0.5	6.5I	 0.07D
	0.5 - 0.55	6.6I	 0.08D
	0.55 - 0.6	6.7I	 0.08D
	0.6 - 0.7	6.8I	 0.08D
	0.7 - 0.8	6.9I	 0.08D
	0.8 - 0.9
	0.9 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.145A	 33C	 50	 7	 7
	0.1 - 0.2	 0.089A
	0.2 - 0.3	 0.043A
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.55	 0.038A	 22C	 39	 4	 34
	0.55 - 0.6
	0.6 - 0.7
	0.7 - 0.8	 0.038A	 11C	 20	 2	 62
	0.8 - 0.9
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.55
	0.55 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SP6	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction