Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SW55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Coppi, John	Locality:
	Date Desc.:	06/07/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 6429   1:100000	Rainfall:	0
	Northing/Long.:	137.658333333333	Runoff:	No Data
	Easting/Lat.:	-34.2666666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Clayey sand; Weak grade of structure, 2-5 mm, 
	Subangular blocky; Weak consistence; 0-2%, coarse fragments; 
	0.1 - 0.2 m	Red (2.5YR5/8-Moist); ; Sandy medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Strong consistence; 0-2%, coarse fragments; 
	0.2 - 0.3 m	Red (2.5YR5/8-Moist); ; Sandy medium clay; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Very strong consistence; 0-2%, coarse fragments; 
	0.3 - 0.4 m	Red (2.5YR5/8-Moist); ; Sandy medium clay; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Very strong consistence; 0-2%, coarse fragments; Soil matrix is Highly calcareous; 
	0.4 - 0.5 m	Red (2.5YR5/8-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular blocky; Firm 
	consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.5 - 0.6 m	Pink (7.5YR8/4-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular blocky; Firm 
	consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.6 - 0.7 m	Pink (7.5YR8/4-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular blocky; Firm 
	consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.7 - 0.8 m	Pink (7.5YR8/4-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular blocky; Firm 
	consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly calcareous; 
	0.8 - 0.9 m	Reddish yellow (7.5YR8/6-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly 
	0.9 - 1 m	Reddish yellow (7.5YR8/6-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Subangular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Nodules; Soil matrix is Highly 
	Morphological Notes
	Observation Notes
	ORIGINALLY SW70/W36; DATA IS FROM BULK OF 8 CORES;                                                                      
	Site Notes
	MAITLAND

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SW55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.2I	 0.26D
	0.1 - 0.2	8.4I	 0.21D
	0.2 - 0.3	8.7I	 0.16D
	0.3 - 0.4	8.9I	 0.14D
	0.4 - 0.5	9.1I	 0.13D
	0.5 - 0.6	9.2I	 0.16D
	0.6 - 0.7	9.5I	 0.21D
	0.7 - 0.8	9.5I	 0.28D
	0.8 - 0.9	9.8I	 0.35D
	0.9 - 1	9.8I	 0.4D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.2C	 0.065A	 28C	 47	 3	 16
	0.1 - 0.2	 8.5C	 0.033A	 22C	 36	 0	 29
	0.2 - 0.3	 21.2C	 0.02A
	0.3 - 0.4	 27.1C
	0.4 - 0.5	 26.5C
	0.5 - 0.6	 24.4C	 0.008A
	0.6 - 0.7	 22.7C
	0.7 - 0.8	 23.5C
	0.8 - 0.9	 24.5C
	0.9 - 1	 24.8C	 0.005A	 19C	 36	 3	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SW55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction