Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SW62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G.C. Kay	Locality:	Cunliffe
	Date Desc.:	29/06/67	Elevation:	No Data
	Map Ref.:	Sheet No. : 738840   1:10000	Rainfall:	No Data
	Northing/Long.:	137.74666666	Runoff:	No Data
	Easting/Lat.:	-34.2333333  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	GC1.22
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Confidence level not specified	soil
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Clay loam; Weak grade of structure; ; ; Gradual change to - 
	B	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Light clay; Moderate grade of structure; 
	0.2 - 0.3 m	Reddish brown (5YR4/3-Moist); , 0-0% ; Light clay; Weak grade of structure; 
	0.3 - 0.4 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Light clay; Weak grade of structure; 
	0.4 - 0.5 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Light clay; Weak grade of structure; 
	Morphological Notes
	Observation Notes
	unpublished; previously SA67/W5; chemistry bulk of 8 cores
	Site Notes

	Project Name:	National Soil Fertility
	Project Code:	NSF	Site ID:	SW62	Observation 	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.5I	0.28D
	0.1 - 0.2	8I	0.23D
	0.2 - 0.3	8.2I	0.27D
	0.3 - 0.4	8.3I	0.32D
	0.4 - 0.5	8.7I	0.45D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.032A	0.113A	1.333B	18C	28	10	36
	0.1 - 0.2	0.8C	0.209A
	0.2 - 0.3	32.6C	0.091A
	0.3 - 0.4	58.7C	0.031A	0.733B	5C	10	6	18
	0.4 - 0.5	58.6C	0.03A	0.058A	0.7B	5C	10	7	18
	Laboratory Analyses Completed for this profile
	10A_NR	Total sulfur - S(%) - Not recorded
	17A_NR	Total element - K (%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded