Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A779	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	31/01/62	Elevation:	 38 metres
	Map Ref.:	Rainfall:	350
	Northing/Long.:	137.622222222222	Runoff:	Rapid
	Easting/Lat.:	-34.1558333333333	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Sand plain
	1-3%
	Morph. Type:	Ridge	Relief:	9 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized 
	Analytical data are incomplete but reasonable confidence.	solonetz
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Yellowish brown (10YR5/4-Moist); ; Sand; Diffuse change to - 
	A	0.1 - 1.5 m	Yellow (10YR7/6-Moist); ; Sand; Abrupt change to - 
	B	1.5 - 2.05 m	Yellowish red (5YR5/8-Moist); ; Clayey sand; Massive grade of structure; Firm consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Abrupt change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	CO DALY

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A779	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.15 - 0.45	9.4H	 0.034C
	1.83 - 2.13	9.4H	 0.025C
	3.35 - 3.65	10.2H	 0.27C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.15 - 0.45	 0.21C	 32C	 64	 0	 4
	1.83 - 2.13	 2.1C	 35C	 56	 0	 6
	3.35 - 3.65	 20C	 30C	 45	 0	 5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.15 - 0.45
	1.83 - 2.13
	3.35 - 3.65

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A779	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded