Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A791	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	06/02/62	Elevation:	 107 metres
	Map Ref.:	Rainfall:	350
	Northing/Long.:	137.983333333333	Runoff:	Rapid
	Easting/Lat.:	-33.9166666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroclcic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Very 
	weak consistence; Diffuse change to - 
	0.08 - 0.25 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Very weak 
	consistence; Diffuse change to - 
	0.25 - 0.4 m	Dark red (2.5YR3/6-Moist); ; Sandy medium clay; Massive grade of structure; Firm consistence; 
	Abrupt change to - 
	0.4 - 0.5 m	; 
	Morphological Notes
	abrupt sheet of very hard kunkar
	Observation Notes
	GRADATIONAL TYPE OF PROFILE:                                                                                            
	Site Notes
	CO DALY

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A791	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.8H	 0.022C
	0.08 - 0.25
	0 - 0.08	7.8H	 0.022C
	0.25 - 0.4
	0.4 - 0.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.02C	 1	 33C	 38	 9	 16
	0.08 - 0.25
	0 - 0.08	 0.02C	 1	 33C	 38	 9	 16
	0.25 - 0.4
	0.4 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.25
	0 - 0.08
	0.25 - 0.4
	0.4 - 0.5

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A791	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded