Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A852	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	10/12/62	Elevation:	 43 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	355
	Northing/Long.:	137.701388888889	Runoff:	Moderately rapid
	Easting/Lat.:	-34.0194444444445	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Triticum aestivum
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.07 m	Brown (10YR5/3-Dry); ; Clay loam; Massive grade of structure; Firm consistence; 0-2%, 
	Gravel, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; Abrupt change
	0.07 - 0.17 m	Reddish brown (5YR4/4-Dry); ; Light clay; Massive grade of structure; Firm consistence; 0-2%,
	 Gravel, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; Abrupt 
	0.17 - 0.43 m	Brown (7.5YR5/4-Dry); ; Light clay; Massive grade of structure; Very weak consistence; 0-2%,
	 Gravel, coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; Diffuse change 
	0.43 - 1.19 m	Pink (7.5YR8/4-Dry); ; Silty loam; Massive grade of structure; Firm consistence; 0-2%, Gravel, 
	coarse fragments; Very many (50 - 100 %), Calcareous, , Soft segregations; Diffuse change to
	1.19 - 1.49 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	WALLAROO

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A852	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.4H	 0.083C
	0.08 - 0.18	8.5H	 0.14C
	0.18 - 0.43	8.8H	 0.41C
	0.53 - 0.61	8.9H	 1C
	0.91 - 1.02	9.1H	 0.21C
	1.19 - 1.49
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 2.2C	 10	 7C	 29	 20	 31
	0.08 - 0.18	 1C	 7C	 29	 14	 41
	0.18 - 0.43	 30C	 7	 4C	 21	 3	 36
	0.53 - 0.61	 50C	 21	 3C	 15	 3	 24
	0.91 - 1.02	 60C	 36	 3C	 14	 3	 15
	1.19 - 1.49
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.18 - 0.43
	0.53 - 0.61
	0.91 - 1.02
	1.19 - 1.49

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A852	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction