Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A854	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	12/12/62	Elevation:	 43 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	355
	Northing/Long.:	137.701388888889	Runoff:	Rapid
	Easting/Lat.:	-34.0194444444445	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Paralithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Triticum aestivum
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.12 m	Reddish brown (5YR4/4-Dry); ; Clay loam; Moderate grade of structure, Angular blocky; Very 
	firm consistence; 0-2%, Gravel, coarse fragments; Sharp change to - 
	0.12 - 0.27 m	Dark reddish brown (2.5YR3/4-Dry); ; Medium clay; Strong grade of structure, Subangular 
	blocky; Very firm consistence; 0-2%, Gravel, coarse fragments; Very few (0 - 2 %), 
	Calcareous, , Concretions; Sharp change to - 
	0.27 - 0.66 m	Reddish yellow (7.5YR7/6-Dry); ; Light clay; Massive grade of structure; Very firm consistence;
	 0-2%, Gravel, coarse fragments; Very many (50 - 100 %), Calcareous, , Soft segregations; 
	Diffuse change to - 
	0.66 - 1.39 m	Pink (5YR8/3-Dry); ; Light clay; Massive grade of structure; Very firm consistence; Very many 
	(50 - 100 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	WALLAROO

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A854	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	8.5H	 0.08C
	0.12 - 0.27	8.5H	 0.073C
	0.27 - 0.66	8.9H	 0.12C
	0.66 - 0.76	9.5H	 0.23C
	1.04 - 1.12	9.9H	 0.24C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	 0.4C	 7C	 28	 12	 44
	0.12 - 0.27	 0.48C	 6C	 28	 11	 48
	0.27 - 0.66	 39C	 3	 3C	 16	 5	 33
	0.66 - 0.76	 58C	 2C	 9	 4	 23
	1.04 - 1.12	 63C	 1C	 7	 4	 21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.27
	0.27 - 0.66
	0.66 - 0.76
	1.04 - 1.12

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A854	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded