Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A856	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	12/12/62	Elevation:	 46 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	355
	Northing/Long.:	137.623611111111	Runoff:	Moderately rapid
	Easting/Lat.:	-34.1305555555556	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Petroclcic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Calcareous sand
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Triticum aestivum
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Pale brown (10YR6/3-Dry); ; Loamy sand; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Diffuse change to - 
	0.1 - 0.48 m	Very pale brown (10YR8/3-Dry); ; Loamy sand; Very many (50 - 100 %), Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.48 - 1.14 m	Very pale brown (10YR8/3-Dry); ; Sandy clay loam; Massive grade of structure; Strong 
	consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Diffuse change to - 
	1.14 - 2.66 m	Yellow (10YR8/6-Dry); ; Sandy clay loam; Massive grade of structure; Strong consistence; 
	Very many (50 - 100 %), Calcareous, , Soft segregations; Calcrete, Very strongly cemented, 
	Discontinuous; 
	2.66 - 2.96 m	; 
	 -  m	; 
	Morphological Notes
	Observation Notes
	2 IRREGULARLY DEVELOPED KUNKAR LAYERS APPROX. 150MM THICK AT DEPTHS 63.5-79CM & 175-190.5CM:                      
	      
	Site Notes
	TIPARRA

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A856	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.7H	 0.054C
	0.25 - 0.33	9H	 0.052C
	0.69 - 0.76	9.5H	 0.065C
	1.14 - 1.22	9.8H	 0.21C
	1.78 - 1.88	9.9H	 0.26C
	2.11 - 2.18	9.9H	 0.24C
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 16C	 4	 30C	 41	 1	 10
	0.25 - 0.33	 30C	 74	 29C	 30	 1	 7
	0.69 - 0.76	 47C	 48	 20C	 24	 2	 8
	1.14 - 1.22	 35C	 11	 22C	 30	 2	 9
	1.78 - 1.88	 27C	 60	 30C	 34	 8
	2.11 - 2.18	 27C	 3	 28C	 37	 0	 8
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.25 - 0.33
	0.69 - 0.76
	1.14 - 1.22
	1.78 - 1.88
	2.11 - 2.18
	 - 

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A856	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded