Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A857	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	12/12/62	Elevation:	 46 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	355
	Northing/Long.:	137.623611111111	Runoff:	Moderately rapid
	Easting/Lat.:	-34.1305555555556	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Petroclcic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Calcareous sand
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Triticum aestivum
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Brown (10YR5/3-Dry); ; Sandy loam; Single grain grade of structure; Very weak consistence; 
	Common (10 - 20 %), Calcareous, , Soft segregations; Sharp change to - 
	0.1 - 0.78 m	Pink (7.5YR7/4-Dry); ; Sandy clay loam; Single grain grade of structure; Firm consistence; Very 
	many (50 - 100 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.78 - 2.28 m	Reddish yellow (7.5YR8/6-Dry); ; Sandy clay loam; Single grain grade of structure; Firm 
	consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Calcrete, Strongly 
	cemented, Discontinuous; 
	2.28 - 2.58 m	; 
	 -  m	; 
	 -  m	; 
	 -  m	; 
	 -  m	; 
	Morphological Notes
	Observation Notes
	KUNKAR LAYERS AT 142-152MM & 185-193MM                                                                                  
	Site Notes
	TIPARRA

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A857	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.7H	 0.045C
	0.23 - 0.3	9H	 0.038C
	0.48 - 0.53	9.1H	 0.042C
	0.91 - 0.99	9.4H	 0.061C
	1.42 - 1.52	9.9H	 0.16C
	1.68 - 1.75	10H	 0.19C
	1.85 - 1.93	10H	 0.22C
	2.18 - 2.26	10.1H	 0.22C
	2.28 - 2.58
	 - 
	 - 
	 - 
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 4.3C	 2	 43C	 37	 2	 11
	0.23 - 0.3	 21C	 4	 31C	 29	 2	 13
	0.48 - 0.53	 27C	 13	 29C	 26	 2	 13
	0.91 - 0.99	 28C	 5	 30C	 23	 1	 14
	1.42 - 1.52	 42C	 68	 23C	 22	 1	 10
	1.68 - 1.75	 32C	 30C	 23	 15
	1.85 - 1.93	 45C	 29	 23C	 17	 1	 14
	2.18 - 2.26	 36C	 27C	 21	 1	 14
	2.28 - 2.58
	 - 
	 - 
	 - 
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.23 - 0.3
	0.48 - 0.53
	0.91 - 0.99
	1.42 - 1.52
	1.68 - 1.75
	1.85 - 1.93
	2.18 - 2.26
	2.28 - 2.58
	 - 
	 - 
	 - 
	 - 

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A857	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded