Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A882	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	01/02/63	Elevation:	 99 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	365
	Northing/Long.:	137.765277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-34.1416666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.07 m	Reddish brown (5YR4/4-Dry); ; Clay loam; Weak grade of structure, Subangular blocky; Very firm 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Diffuse change to - 
	B	0.07 - 0.27 m	Red (2.5YR4/6-Dry); ; Light clay; Strong grade of structure, Subangular blocky; Very firm 
	consistence; Diffuse change to - 
	Bk	0.27 - 0.6 m	Reddish yellow (7.5YR7/6-Dry); ; Medium clay; Massive grade of structure; Very firm 
	consistence; Common (10 - 20 %), Calcareous, , Concretions; Diffuse change to - 
	0.6 - 1.09 m	Pink (5YR8/3-Dry); ; Medium clay; Massive grade of structure; Strong consistence; Many (20 - 50 
	%), Calcareous, , Soft segregations; Diffuse change to - 
	1.09 - 1.67 m	Light red (2.5YR6/6-Dry); ; Weak grade of structure, Subangular blocky; Strong consistence; 
	Many (20 - 50 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	TIPARRA

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A882	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	8.4H	 0.071C
	0.07 - 0.27	8.4H	 0.054C
	0.27 - 0.6	9.1H	 0.062C
	0.6 - 1.09	9.8H	 0.13C
	1.35 - 1.47	9.9H	 0.17C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	 13C	 5	 15C	 28	 14	 26
	0.07 - 0.27	 0.22C	 3	 14C	 23	 12	 47
	0.27 - 0.6	 52C	 41	 6C	 11	 3	 23
	0.6 - 1.09	 65C	 4	 4C	 9	 3	 15
	1.35 - 1.47	 32C	 18	 6C	 22	 9	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.27
	0.27 - 0.6
	0.6 - 1.09
	1.35 - 1.47

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A882	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded