Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A885	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	01/02/63	Elevation:	 38 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	355
	Northing/Long.:	137.593055555556	Runoff:	Moderately rapid
	Easting/Lat.:	-34.1430555555556	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Hypocalcic Yellow Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.07 m	Pale brown (10YR6/3-Dry); ; Sand; Loose consistence; Sharp change to - 
	A1	0.07 - 0.12 m	Very pale brown (10YR7/4-Dry); ; Sand; Very weak consistence; Diffuse change to - 
	A2	0.12 - 0.15 m	Very pale brown (10YR7/3-Dry); ; Sand; Loose consistence; Sharp change to - 
	B1	0.15 - 0.22 m	Reddish yellow (7.5YR6/6-Dry); ; Loamy sand; Massive grade of structure; Very firm 
	consistence; Diffuse change to - 
	B2	0.22 - 0.33 m	Yellow (10YR7/6-Dry); , 5YR46; Sandy clay loam; Massive grade of structure; Very firm 
	consistence; Calcrete; Diffuse change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	TIPARRA

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A885	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	8.3H	 0.015C
	0.07 - 0.12	8.6H	 0.018C
	0.12 - 0.15	8.6H	 0.017C
	0.15 - 0.22	8.2H	 0.028C
	0.22 - 0.33	8.6H	 0.059C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	<0.01C	 56C	 41	 1	 2
	0.07 - 0.12	 0.02C	 43C	 51	 0	 4
	0.12 - 0.15	 0.01C	 49C	 48	 1	 2
	0.15 - 0.22	 0.03C	 31C	 50	 2	 14
	0.22 - 0.33	 0.11C	 40C	 33	 0	 23
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.12
	0.12 - 0.15
	0.15 - 0.22
	0.22 - 0.33

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A885	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded