Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A919	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	04/09/63	Elevation:	 96 metres
	Map Ref.:	Sheet No. : SI53-12   1:250000	Rainfall:	365
	Northing/Long.:	137.684722222222	Runoff:	Rapid
	Easting/Lat.:	-34.1583333333334	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	8 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Regolithic Bleached Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - , , . *Species includes - Triticum aestivum
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.07 m	Very dark brown (10YR2/3-Moist); ; Fine sand; Sharp change to - 
	0.07 - 0.12 m	Reddish yellow (7.5YR6/6-Moist); ; Fine sand; Sharp change to - 
	0.12 - 0.25 m	Very pale brown (10YR7/4-Moist); ; Fine sand; Sharp change to - 
	0.25 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Fine sand; Sharp change to - 
	0.3 - 0.6 m	Reddish yellow (7.5YR6/6-Moist); ; Fine sand; Diffuse change to - 
	0.6 - 1.21 m	Reddish yellow (7.5YR7/6-Moist); , 5YR58; Fine sand; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Abrupt change to - 
	1.21 - 1.44 m	; Loamy fine sand; Massive grade of structure; Weak consistence; Diffuse change to - 
	1.44 - 1.82 m	Very pale brown (10YR8/4-Moist); ; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	LAYER 7 - SLIGHTLY LOAMY WEAKLY INDURATED KUNKAR                                                                        
	Site Notes
	TIPARRA

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A919	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	7.1H	 0.03C
	0.07 - 0.12	7.7H	 0.022C
	0.12 - 0.25	7.7H	 0.01C
	0.25 - 0.3	8.1H	 0.015C
	0.3 - 0.6	8.1H	 0.017C
	0.6 - 1.21	8.8H	 0.032C
	1.21 - 1.44
	1.44 - 1.82	9.4H	 0.036C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	 0.02C	 27C	 69	 0	 6
	0.07 - 0.12	 0.02C	 35C	 58	 0	 6
	0.12 - 0.25	 0.01C	 32C	 64	 0	 4
	0.25 - 0.3	<0.01C	 33C	 61	 0	 6
	0.3 - 0.6	<0.01C	 27C	 64	 0	 9
	0.6 - 1.21	 0.96C	 29C	 59	 0	 11
	1.21 - 1.44
	1.44 - 1.82	 16C	 26C	 52	 0	 6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.12
	0.12 - 0.25
	0.25 - 0.3
	0.3 - 0.6
	0.6 - 1.21
	1.21 - 1.44
	1.44 - 1.82

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A919	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded