Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A941	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	27/10/64	Elevation:	 5 metres
	Map Ref.:	Rainfall:	360
	Northing/Long.:	137.519166666667	Runoff:	Rapid
	Easting/Lat.:	-34.1436111111111	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Sand plain
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Regolithic Calcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Calcareous sand
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.38 m	Brown (10YR4/3-Moist); ; Sand; Common (10 - 20 %), Calcareous, , Soft segregations; Diffuse 
	change to - 
	0.38 - 1.05 m	Brown (7.5YR5/4-Moist); ; Sand; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.05 - 1.35 m	; 
	 -  m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	DALY

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A941	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	9H	 0.034C
	0.15 - 0.38	9H	 0.035C
	0.38 - 0.76	9.1H	 0.046C
	0.91 - 1.07	9.7H	 0.055C
	1.05 - 1.35
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 31C	 0.077B	 20C	 39	 1	 4
	0.15 - 0.38	 32C	 2C	 57	 4
	0.38 - 0.76	 24C	 29C	 39	 5
	0.91 - 1.07	 24C	 14C	 55	 4
	1.05 - 1.35
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.38
	0.38 - 0.76
	0.91 - 1.07
	1.05 - 1.35
	 - 

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A941	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded