Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:	IN COAST CLIFF AT HARRY'S POINT - MOONTA 
	BAY:
	Date Desc.:	27/07/65	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	137.5583333	Runoff:	No Data
	Easting/Lat.:	-34.0633333333333	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red clay
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	; Medium clay; 
	0.03 - 0.3 m	; Medium clay; 
	0.3 - 0.6 m	; Medium clay; 
	0.6 - 0.9 m	; Medium clay; 
	0.9 - 1.2 m	; Medium clay; 
	1.2 - 1.5 m	; Medium clay; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	8.1H	 1.9C
	0.03 - 0.3	5.8H	 1.8C
	0.3 - 0.6	5.5H	 1.3C
	0.6 - 0.9	5.2H	 2.7C
	0.9 - 1.2	5.6H	 2.9C
	1.2 - 1.5	6.4H	 2.5C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.096C	 25C	 44	 1	 26
	0.03 - 0.3	 24C	 37	 2	 35
	0.3 - 0.6	 17C	 39	 4	 39
	0.6 - 0.9	 21C	 37	 3	 37
	0.9 - 1.2	 20C	 39	 3	 35
	1.2 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	Upper York Penin., S.A.
	Project Code:	NY1	Site ID:	A958	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	MIN_NR_K2O	Kaolin minerals
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction