Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A576	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	23/09/58	Elevation:	 120 metres
	Map Ref.:	Sheet No. : SJ54-2   1:250000	Rainfall:	560
	Northing/Long.:	140.7313889	Runoff:	Rapid
	Easting/Lat.:	-36.92611111	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	24 metres
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Fragic Sesquic Aeric Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - Themeda triandra
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, . *Species includes - Eucalyptus baxteri
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Greyish brown (10YR5/2-Moist); ; Sand; , Granular; Moist; Weak consistence; Slightly plastic; 
	Few, very fine (0-1mm) roots; 
	A1B	0.04 - 0.08 m	Greyish brown (10YR5/2-Moist); ; Sand; , Granular; Moist; Weak consistence; Slightly plastic; 
	Common, fine (1-2mm) roots; 
	A1C	0.08 - 0.25 m	Greyish brown (10YR5/2-Moist); Light brownish grey (10YR6/2-Moist); ; Sand; , Granular; Moist; 
	Weak consistence; Slightly plastic; Abundant, medium (2-5mm) roots; 
	0.3 - 0.55 m	Light brownish grey (10YR6/2-Moist); Yellowish brown (10YR5/4-Moist); ; Sand; Loose 
	consistence; Abundant, very fine (0-1mm) roots; 
	0.55 - 0.94 m	White (10YR8/2-Moist); ; Sand; Loose consistence; , very fine (0-1mm) roots; 
	0.94 - 1.32 m	White (10YR8/2-Moist); ; Sand; Loose consistence; 
	B	1.6 - 2.03 m	Yellowish brown (10YR5/4-Moist); , 10YR68; , 7.5YR44; Sand; Moist; Loose consistence; 
	2.26 - 2.62 m	Brownish yellow (10YR6/8-Moist); ; Sand; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	CO. ROBE Div. Soils Div. Report 4/65 p32

	Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A576	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.2H	 0.009C
	0.04 - 0.08	6H	 0.01C
	0.08 - 0.25	5.5H	 0.006C
	0.3 - 0.55	5.6H	 0.003C
	0.55 - 0.94	5.7H	 0.003C
	0.94 - 1.32	5.8H	 0.002C
	1.6 - 2.03	5.6H	 0.005C
	2.26 - 2.62	6.3H	 0.004C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.036B	 90C	 7	 1	 0
	0.04 - 0.08
	0.08 - 0.25	 0.025B
	0.3 - 0.55
	0.55 - 0.94
	0.94 - 1.32	 82C	 15	 1	 1
	1.6 - 2.03
	2.26 - 2.62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.08
	0.08 - 0.25
	0.3 - 0.55
	0.55 - 0.94
	0.94 - 1.32
	1.6 - 2.03
	2.26 - 2.62

	Project Name:	Co. Robe Rec. & MacDonnell, S.A.
	Project Code:	RM1	Site ID:	A576	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded