Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	01/11/88	Elevation:	No Data
	Map Ref.:	Sheet No. : 6629-18   1:10000	Rainfall:	No Data
	Northing/Long.:	6217100 AMG zone: 54	Runoff:	No Data
	Easting/Lat.:	289380  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Clay loam, fine sandy; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Dry; Very firm consistence; 2-10%, medium gravelly, 6-
	20mm, subrounded tabular, dispersed, Shale, coarse fragments; Field pH 7 (Raupach); Abrupt 
	change to - 
	A12	0.1 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam, fine sandy; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Dry; Very firm consistence; 2-10%, medium gravelly, 6-
	20mm, subrounded tabular, dispersed, coarse fragments; Field pH 7 (Raupach); Abrupt change 
	to - 
	B21	0.15 - 0.2 m	Reddish brown (2.5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular
	 blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of ped faces or 
	walls coated; Field pH 7 (Raupach); 
	B21	0.2 - 0.3 m	Reddish brown (2.5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of ped faces or 
	walls coated; Field pH 7 (Raupach); 
	B21	0.3 - 0.4 m	Reddish brown (2.5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Smooth-ped fabric; Dry; Strong consistence; Common cutans, 10-50% of ped faces or 
	walls coated; Field pH 7 (Raupach); Clear change to - 
	B22	0.4 - 0.5 m	Reddish brown (2.5YR4/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 50-90%, angular platy, stratified, 
	Shale, coarse fragments; Common cutans, 10-50% of ped faces or walls coated; Common (10 -
	 20 %), Calcareous, Very coarse (20 - 60 mm), Soft segregations; Field pH 8 (Raupach); 
	B22	0.5 - 0.7 m	Reddish brown (2.5YR4/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 50-90%, angular platy, stratified, 
	Shale, coarse fragments; Common cutans, 10-50% of ped faces or walls coated; Many (20 - 50 
	%), Calcareous, Very coarse (20 - 60 mm), Soft segregations; Field pH 8 (Raupach); Gradual 
	change to - 
	BC	0.7 - 1.1 m	Yellowish red (5YR4/6-Moist); , 20-50% , 30-mm, Prominent; Moderate grade of structure, 20-50 
	mm, Angular blocky; Rough-ped fabric; Dry; Strong consistence; 50-90%, angular platy, 
	stratified, Shale, coarse fragments; Few cutans, <10% of ped faces or walls coated; Many (20 - 
	50 %), Calcareous, Fine (0 - 2 mm), Soft segregations; Very few (0 - 2 %), Ferromanganiferous, 
	Fine (0 - 2 mm), Nodules; Field pH 9 (Raupach); Gradual change to - 

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	C	1.1 - 1.5 m	; Rough-ped fabric; 50-90%, angular platy, stratified, Shale, coarse fragments; Many (20 - 50 %), 
	Calcareous, Very coarse (20 - 60 mm), Soft segregations; Field pH 9 (Raupach); Diffuse change
	 to - 
	R	1.5 -  m	Rock 
	Morphological Notes
	A11	Common to upper-slopes and crests.  RBE into WFS.
	B21	The B2 has a moderate to low sorptivity.
	BC	The yellower BC is similar to many other B3's in the catchment - tough and carbonate 
	rich.  The 5yr46 colour is in bands and its mottles are red, grey and white.
	C	C is complex with clay, carbonate and fresh rock bands.
	Observation Notes
	Site Notes

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 1.1
	1.1 - 1.5
	1.5 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 1.1
	1.1 - 1.5
	1.5 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.7
	0.7 - 1.1
	1.1 - 1.5
	1.5 - 

	Project Name:	Rhynie Soil Survey
	Project Code:	Rhynie	Site ID:	A1262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile