Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A822	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	30/05/62	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	140.45	Runoff:	Rapid
	Easting/Lat.:	-36.71666667	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Beach ridge	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sedge, , . *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	; Sand; 
	0.03 - 0.1 m	; Loamy sand; , Columnar; Weak consistence; 
	0.1 - 0.23 m	; Sandy loam; Few (2 - 10 %), Calcareous, , Concretions; 
	0.28 - 0.4 m	; Loam; Common (10 - 20 %), Calcareous, , Concretions; 
	0.4 - 0.48 m	; Sandy clay loam; Common (10 - 20 %), Calcareous, , Concretions; 
	Morphological Notes
	Observation Notes
	Site Notes
	CHANDOS

	Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A822	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	8H	 0.014C
	0.03 - 0.1	8.3H	 0.019C
	0.1 - 0.23	8.8H	 0.032C
	0.28 - 0.4	9H	 0.033C
	0.4 - 0.48	9H	 0.031C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.03C	 56C	 39	 1	 5
	0.03 - 0.1	 0.05C	 42C	 48	 0	 9
	0.1 - 0.23	 5.4C	 45	 34C	 44	 1	 13
	0.28 - 0.4	 12C	 4	 34C	 36	 2	 14
	0.4 - 0.48	 13C	 6	 35C	 36	 0	 14
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.23
	0.28 - 0.4
	0.4 - 0.48

	Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A822	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded