Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A960	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	25/08/65	Elevation:	 49 metres
	Map Ref.:	Rainfall:	330
	Northing/Long.:	141.95	Runoff:	Moderately rapid
	Easting/Lat.:	-35.4	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Low hills
	Morph. Type:	Closed Depression	Relief:	46 metres
	Elem. Type:	Lagoon	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Regolithic Calcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	; Silty loam; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.05 - 0.15 m	; Silty loam; , Angular blocky; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft 
	segregations; 
	0.15 - 0.2 m	; Silty loam; Weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.21 - 0.38 m	; Silty loam; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.38 - 0.58 m	; Silty loam; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Few (2 - 10 %), 
	Gypseous, , ; 
	0.58 - 0.8 m	; Silty loam; Few (2 - 10 %), Calcareous, , Soft segregations; Few (2 - 10 %), Gypseous, , ; 
	0.85 - 1.13 m	; Medium clay; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	1.13 - 1.31 m	; Medium clay; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	1.31 - 1.61 m	; Medium clay; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	1.61 - 1.76 m	; Medium clay; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	1.8 - 2 m	; Medium clay; Common (10 - 20 %), Gypseous, , Crystals; 
	2 - 2.15 m	; Medium clay; Common (10 - 20 %), Gypseous, , Crystals; Abundant, fine (1-2mm) roots; 
	2.15 - 2.55 m	; Medium clay; Common (10 - 20 %), Gypseous, , Crystals; 
	2.55 - 2.75 m	; Medium clay; 
	Morphological Notes
	Observation Notes
	21-58CM WHITE FLECKS POSSIBLY GYPSUM:                                                                                   
	Site Notes
	WEEAH

	Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A960	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.9H	 0.21C
	0.05 - 0.15	8.3H	 0.095C
	0.15 - 0.2	8.2H	 0.63C
	0.21 - 0.38	8H
	0.38 - 0.58	8H
	0.58 - 0.8	8.1H
	0.85 - 1.13	8.2H
	1.13 - 1.31	8.2H	 4.5C
	1.31 - 1.61	8.2H	 3.2C
	1.61 - 1.76	8.6H	 2.7C
	1.8 - 2	8.2H
	2 - 2.15	8.3H
	2.15 - 2.55	8.4H
	2.55 - 2.75	8.3H	 4.8C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 20C	 0.23B
	0.05 - 0.15	 25C	 4C	 8	 7	 53
	0.15 - 0.2	 38C
	0.21 - 0.38	 15C
	0.38 - 0.58	 19C
	0.58 - 0.8	 7.8C
	0.85 - 1.13	 9.2C
	1.13 - 1.31	 22C
	1.31 - 1.61	 24C
	1.61 - 1.76	 25C
	1.8 - 2	 17C
	2 - 2.15	 12C
	2.15 - 2.55	 6.9C
	2.55 - 2.75	 26C	 4C	 7	 10	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.15
	0.15 - 0.2
	0.21 - 0.38
	0.38 - 0.58
	0.58 - 0.8
	0.85 - 1.13
	1.13 - 1.31
	1.31 - 1.61
	1.61 - 1.76
	1.8 - 2
	2 - 2.15
	2.15 - 2.55
	2.55 - 2.75

	Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A960	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)

	Project Name:	Southern Merray Basin
	Project Code:	SMB	Site ID:	A960	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded