Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Locality:	SECOND VALLEY PINE PLANTATION
	Date Desc.:	15/07/59	Elevation:	 305 metres
	Map Ref.:	Rainfall:	760
	Northing/Long.:	138.233333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.5666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plateau
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 6.01-12m, . *Species includes - Pinus radiata
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Brown (10YR4/3-Moist); ; Loam; Weak grade of structure, Granular; Very weak consistence; 2-
	10%, Gravel, coarse fragments; 
	0.03 - 0.13 m	Brown (7.5YR4/4-Moist); ; Clay loam; Weak grade of structure, Granular; Very weak consistence;
	 2-10%, Gravel, coarse fragments; 
	0.13 - 0.3 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Weak grade of structure, Granular; Very weak 
	consistence; 2-10%, Gravel, coarse fragments; 
	0.3 - 0.48 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Weak grade of structure, Granular; Very weak 
	consistence; 2-10%, Gravel, coarse fragments; 
	0.48 - 0.66 m	Strong brown (7.5YR5/6-Moist); , 10YR64; , 5YR46; Medium clay; Very weak consistence; 10-
	20%, Gravel, coarse fragments; 
	0.66 - 1.2 m	Reddish yellow (7.5YR6/8-Moist); , 10YR82; , 10YR46; 50-90%, Gravel, coarse fragments; 
	1.2 - 1.5 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	CAPE JERVIS

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0 - 0.1	5.9H	 0.022C	 6.5K	 3.1	 0.41	 0.29
	0.1 - 0.25	6.5H	 0.012C
	0.25 - 0.46	6.2H	 0.013C
	0.46 - 0.53	5.9H	 0.017C	 1.9K	 7.1	 0.29	 0.52
	0.53 - 0.61	5.9H	 0.017C
	0.61 - 0.91	5.7H	 0.02C	 1.1K	 6.3	 0.16	 0.65
	0.91 - 1.22	5.3H	 0.025C
	1.2 - 1.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0 - 0.1	 4.9E	 0.01F	 0.17B	 0.1B	 38	 19	 15
	0.1 - 0.25	 0.056B	 41	 12	 34
	0.25 - 0.46	 0.01F	 0.066B	 0.17B
	0.46 - 0.53	 1E	 0.057B	 30	 8	 59
	0.53 - 0.61
	0.61 - 0.91	 0.024B	 52	 6	 65
	0.91 - 1.22
	1.2 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.46
	0.46 - 0.53
	0.53 - 0.61
	0.61 - 0.91
	0.91 - 1.22
	1.2 - 1.5

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded