Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Locality:	SECOND VALLEY PINE PLANTATION
	Date Desc.:	15/07/59	Elevation:	 305 metres
	Map Ref.:	Rainfall:	760
	Northing/Long.:	138.233333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.5666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plateau
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 6.01-12m, . *Species includes - Pinus radiata
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Brown (7.5YR4/4-Moist); ; Loam; Weak grade of structure, Granular; Very weak consistence; 2-
	10%, Gravel, coarse fragments; Diffuse change to - 
	0.03 - 0.1 m	Strong brown (7.5YR5/6-Moist); ; Loam; Weak grade of structure, Granular; Very weak 
	consistence; 2-10%, Gravel, coarse fragments; Diffuse change to - 
	0.1 - 0.2 m	Strong brown (7.5YR5/8-Dry); ; Medium clay; Weak grade of structure, Granular; Very weak 
	consistence; 2-10%, Gravel, coarse fragments; Diffuse change to - 
	0.2 - 0.45 m	Brownish yellow (10YR6/6-Dry); ; Medium clay; Weak grade of structure, Granular; 2-10%, Gravel,
	 coarse fragments; Diffuse change to - 
	0.45 - 0.93 m	; Medium clay; 20-50%, Gravel, coarse fragments; Diffuse change to - 
	0.93 - 1.08 m	Pale yellow (2.5Y8/4-Dry); , 10YR66; , 2.5YR34; Diffuse change to - 
	1.08 - 1.38 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	CAPE JERVIS

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0 - 0.1	6.1H	 0.047C	 4.4K	 3.4	 0.62	 1
	0.1 - 0.25	6H	 0.029C
	0.25 - 0.46	6H	 0.021C
	0.46 - 0.53	5.8H	 0.025C
	0.53 - 0.61	5.6H	 0.025C	 1.3K	 5.8	 0.18	 0.54
	0.61 - 0.91	5.3H	 0.026C
	0.91 - 1.19	5.3H	 0.031C	 0.5K	 4	 0.1	 0.6
	1.08 - 1.38
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0 - 0.1	 3.1E	 0.011F	 0.088B	 0.12B	 44	 20	 16
	0.1 - 0.25	 0.049B	 32	 14	 30
	0.25 - 0.46	 0.01F	 0.057B	 0.2B	 29	 9	 48
	0.46 - 0.53
	0.53 - 0.61	 0.39E	 0.03B	 61	 4	 70
	0.61 - 0.91
	0.91 - 1.19	 0.011B	 55	 7	 57
	1.08 - 1.38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.46
	0.46 - 0.53
	0.53 - 0.61
	0.61 - 0.91
	0.91 - 1.19
	1.08 - 1.38

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded