Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A685	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Locality:	SECOND VALLEY PINE PLANTATION
	Date Desc.:	15/07/59	Elevation:	 305 metres
	Map Ref.:	Rainfall:	760
	Northing/Long.:	138.233333333333	Runoff:	Rapid
	Easting/Lat.:	-35.5666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 6.01-12m, . *Species includes - Pinus radiata
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Yellowish red (5YR5/6-Dry); ; Loam; , Granular; Very weak consistence; 2-10%, Gravel, coarse 
	fragments; Diffuse change to - 
	0.03 - 0.23 m	Pink (7.5YR7/4-Dry); ; Loam; , Granular; Very weak consistence; 2-10%, dispersed, Gravel, 
	coarse fragments; Diffuse change to - 
	0.23 - 0.58 m	Red (2.5YR4/8-Dry); ; Medium clay; Strong consistence; Moderately plastic; 2-10%, dispersed, 
	Gravel, coarse fragments; Diffuse change to - 
	0.58 - 0.98 m	Strong brown (7.5YR5/6-Moist); , 5YR56; , 10YR86; Medium clay; Massive grade of structure; 
	Strong consistence; Moderately plastic; 2-10%, dispersed, Gravel, coarse fragments; Diffuse 
	change to - 
	0.98 - 1.55 m	Reddish yellow (7.5YR7/8-Moist); , 10R36; Massive grade of structure; Very weak consistence; 
	Diffuse change to - 
	1.55 - 1.85 m	; 
	 -  m	; 
	Morphological Notes
	Observation Notes
	GRAVEL PROBABLY TRANSPORTED MATERIAL FROM NEARBY LATERITE SURFACE: PROFILE FROMED ON MOTTLED 
	ZONE MATERIAL:             
	Site Notes
	CAPE JERVIS

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A685	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0 - 0.13	6.4H	 0.04C
	0.13 - 0.25	6.2H	 0.023C
	0.25 - 0.46	5.9H	 0.028C
	0.46 - 0.53	5.6H	 0.026C
	0.53 - 0.61	5.5H	 0.026C
	0.61 - 0.91	5.5H	 0.021C
	0.91 - 1.22	5.5H	 0.018C
	1.55 - 1.85
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0 - 0.13	 3.1E	 0.008F	 0.092B	 0.09B	 37	 19	 12
	0.13 - 0.25	 0.047B	 23	 19	 20
	0.25 - 0.46	 0.01F	 0.033B	 0.1B	 13	 15	 43
	0.46 - 0.53
	0.53 - 0.61	 0.34E	 0.013B	 5	 17	 41
	0.61 - 0.91
	0.91 - 1.22	 0.004B	 4	 24	 22
	1.55 - 1.85
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0 - 0.13
	0.13 - 0.25
	0.25 - 0.46
	0.46 - 0.53
	0.53 - 0.61
	0.61 - 0.91
	0.91 - 1.22
	1.55 - 1.85
	 - 

	Project Name:	Second Valley Pine Plantation, S.A.
	Project Code:	SVP	Site ID:	A685	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded