Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A90	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:	SOME INCIPIENT GULLYING OCCURS ON SIMILAR 
	HILLS
	Date Desc.:	09/06/54	Elevation:	 130 metres
	Map Ref.:	1:250000	Rainfall:	470
	Northing/Long.:	140.908055555556	Runoff:	Moderately rapid
	Easting/Lat.:	-36.3227777777778	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Red Sodosol     	Principal Profile Form:	Dr2.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - Danthonia species
	Tall Strata - , , . *Species includes - Eucalyptus odorata, Melaleuca unicinata
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Yellowish red (5YR4/6-Moist); ; Loamy sand; Very weak consistence; 
	0.08 - 0.1 m	Very pale brown (10YR7/4-Moist); ; Sand; Very firm consistence; 
	0.1 - 0.2 m	Red (2.5YR4/6-Moist); ; Medium clay; , Columnar; Strong consistence; 
	0.3 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Very firm consistence; 
	0.46 - 0.56 m	Yellowish red (5YR5/8-Moist); ; Medium clay; Very weak consistence; Common (10 - 20 %), 
	Calcareous, , Soft segregations; 
	0.91 - 0.97 m	Yellowish red (5YR5/8-Moist); ; Sandy medium clay; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	LIME FROM 46 CM: LAYERS RENUMBERED 10/11/92                                                                             
	Site Notes
	BUCKINGHAM

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A90	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.7A	 0.013C
	0.08 - 0.1	6.6A	 0.013C
	0.1 - 0.2
	0.1 - 0.46	7.5A	 0.063C
	0.46 - 0.56	9.4A	 0.32C
	0.91 - 0.97	9.1A	 0.38C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.1
	0.1 - 0.2
	0.1 - 0.46
	0.46 - 0.56
	0.91 - 0.97
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.1
	0.1 - 0.2
	0.1 - 0.46
	0.46 - 0.56
	0.91 - 0.97

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A90	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour