Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:	UNCLEARED VIRGIN SITE WITH FAIR GRASS 
	COVER
	Date Desc.:	10/06/54	Elevation:	 110 metres
	Map Ref.:	1:250000	Rainfall:	480
	Northing/Long.:	140.847777777778	Runoff:	Very slow
	Easting/Lat.:	-36.3583333333333	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Crusty Grey Vertosol     	Principal Profile Form:	Dy2.13
	ASC Confidence:	Great Soil Group:	Solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Casuarina leuhmannii
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Grey (10YR5/1-Moist); ; Sandy loam; 
	0.03 - 0.13 m	Grey (10YR5/1-Moist); ; Medium clay; Massive grade of structure; 
	0.13 - 0.38 m	Grey (10YR5/1-Moist); ; Medium clay; Moderately plastic; Normal plasticity; 
	0.38 - 0.61 m	Grey (10YR5/1-Moist); ; Medium clay; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.56 - 0.61 m	Grey (10YR5/1-Moist); ; Medium clay; Few (2 - 10 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	LIME FROM 46 CM: LAYERS RENUMBERED 10/11/92                                                                             
	Site Notes
	BUCKINGHAM

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	7.2A	 0.035C
	0.03 - 0.13	8A	 0.041C
	0.13 - 0.38
	0.38 - 0.61
	0.56 - 0.61	9.5A	 0.35C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.007F	 0.18B
	0.03 - 0.13
	0.13 - 0.38
	0.38 - 0.61
	0.56 - 0.61	 0.004F	 0.43B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.13
	0.13 - 0.38
	0.38 - 0.61
	0.56 - 0.61

	Project Name:	Tatiara, S.A.
	Project Code:	TA1	Site ID:	A98	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	9A_NR	Total element - P(%) - Not recorded