Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	012	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	14/11/90	Elevation:	432 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6151720 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	315120  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1 m deep,No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Recently cultivated
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.12
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Confidence level not specified	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.3 m	Brown (7.5YR5/2-Moist); , 0-0% ; Sandy loam; Single grain grade of structure; Dry; Loose 
	consistence; Clear, Smooth change to - 
	Bt	0.3 - 0.8 m	Strong brown (7.5YR5/8-Moist); , 2.5YR48, 10-20% , 5-15mm, Distinct; Heavy clay; Single grain 
	grade of structure; Loose consistence; Diffuse, Smooth change to - 
	BC	0.8 - 1.2 m	White (5YR8/1-Moist); , 7.5YR58, 10-20% , 5-15mm, Distinct; , 2.5YR48; Medium heavy clay; 
	Single grain grade of structure; Moist; Loose consistence; Gradual, Smooth change to - 
	C	1.2 -  m	Strong brown (7.5YR5/8-Moist); , 2.5YR48, 10-20% , 5-15mm, Distinct; Sandy clay loam; Single 
	grain grade of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	012	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	012	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile