Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	14/11/90	Elevation:	475 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6152100 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	318410  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1 m deep,Slightly porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	350 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.11
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Confidence level not specified	soil
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	O	0 - 0.04 m	Organic Layer; , 0-0% ; Loamy sand; Single grain grade of structure; Loose consistence; Sharp, 
	Smooth change to - 
	A1	0.04 - 0.5 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Loose 
	consistence; Clear, Smooth change to - 
	Btg	0.5 - 0.6 m	Dark greyish brown (10YR4/2-Moist); , 2.5R36, 2-10% , 5-15mm, Distinct; , 7.5YR58; Medium 
	heavy clay; Single grain grade of structure; Moderately moist; Loose consistence; Clear, 
	Smooth change to - 
	BCg	0.6 - 0.75 m	Dark greyish brown (10YR4/2-Moist); , 2.5R36, 20-50% , 5-15mm, Distinct; Medium clay; Single 
	grain grade of structure; Moist; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	020	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile