Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	048	Observation ID:	2
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	28/11/90	Elevation:	424 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6157390 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	319760  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 3 m deep,Porous, Clay 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Peneplain
	1-3%
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O	0 - 0.03 m	Organic Layer; , 0-0% ; Single grain grade of structure; Dry; Loose consistence; Abrupt, Smooth 
	change to - 
	A1	0.03 - 0.5 m	Greyish brown (10YR5/2-Moist); White (10YR8/2-Dry); , 0-0% ; Loamy sand; Single grain grade of
	 structure; Moderately moist; Loose consistence; Clear, Smooth change to - 
	A2	0.5 - 1 m	Brownish yellow (10YR6/6-Moist); Very pale brown (10YR7/4-Dry); , 0-0% ; Clayey sand; Single 
	grain grade of structure; Moist; Loose consistence; Gradual, Smooth change to - 
	Bt	1 - 1.3 m	Light grey (10YR7/1-Moist); , 7.5YR58, 10-20% , 5-15mm, Distinct; , 5YR58; Sandy clay; Single 
	grain grade of structure; Wet; Loose consistence; Gradual, Smooth change to - 
	Bt	1.3 - 1.5 m	Light grey (2.5Y7/0-Moist); , 10R48, 10-20% , 5-15mm, Distinct; , 7.5YR58; Light clay; Single 
	grain grade of structure; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	A1414

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	048	Observation ID:	2
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	048	Observation ID:	2
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile