Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1101	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	B. Purdie	Locality:
	Date Desc.:	20/04/98	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6495930 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	424903  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling hills 90-300m 10-32%	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	12 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting
	Erosion:	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol     	Principal Profile Form:	Uf6.22
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 
	Profile 
	A1	0 - 0.24 m	Dark reddish brown (5YR3/3-Moist); ; Light medium clay; Weak grade of structure, 2-5 mm, Subangular 
	blocky; Earthy fabric; Moist; 2-10%, coarse fragments; Field pH 6.9 (pH meter); Common, fine (1-2mm) 
	roots; Clear, Smooth change to - 
	B21t	0.24 - 0.6 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, Angular blocky; 
	Moderately moist; 2-10%, coarse fragments; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Field pH 6.6 (pH meter); Few, coarse (>5mm) roots; Clear, Wavy change to - 
	B22t	0.6 - 0.9 m	Brown (7.5YR4/4-Moist); ; Medium heavy clay; Weak grade of structure, 100-200 mm, Angular blocky; 
	Moderately moist; 20-50%, cobbly, 60-200mm, angular tabular, Dolerite, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; Field pH 6.4 (pH meter); Few, coarse (>5mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	Photos Roll 57/23 & 25.

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1101	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.24	5.6B	4B	6.94A	7.14	0.49	0.32	14.89D
	6.8H
	0 - 0.24	5.6B	4B	6.94A	7.14	0.49	0.32	14.89D
	6.8H
	0 - 0.24	5.6B	4B	6.94A	7.14	0.49	0.32	14.89D
	6.8H
	0.12 - 0.17
	0.24 - 0.6	5.2B	2B	7.72A	12.79	0.35	0.66	21.52D
	6.8H
	0.24 - 0.6	5.2B	2B	7.72A	12.79	0.35	0.66	21.52D
	6.8H
	0.24 - 0.6	5.2B	2B	7.72A	12.79	0.35	0.66	21.52D
	6.8H
	0.26 - 0.31
	0.6 - 0.9	5.4B	7B	7.62A	13.06	0.21	1.34	22.23D
	6.7H
	0.6 - 0.9	5.4B	7B	7.62A	13.06	0.21	1.34	22.23D
	6.7H
	0.6 - 0.9	5.4B	7B	7.62A	13.06	0.21	1.34	22.23D
	6.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.24	1.25D	120B	0.073E	11.6	18.3
	0 - 0.24	1.25D	120B	0.073E	11.6	18.3
	0 - 0.24	1.25D	120B	0.073E	11.6	18.3
	0.12 - 0.17	1.20
	0.24 - 0.6	0.34D	51B	0.035E	13.8	19.9
	0.24 - 0.6	0.34D	51B	0.035E	13.8	19.9
	0.24 - 0.6	0.34D	51B	0.035E	13.8	19.9
	0.26 - 0.31	1.40
	0.6 - 0.9	0.23D	48B	0.032E	9.5	17.6
	0.6 - 0.9	0.23D	48B	0.032E	9.5	17.6
	0.6 - 0.9	0.23D	48B	0.032E	9.5	17.6
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1101	Observation 	1
	Agency Name:	Agriculture Western Australia
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_20_100	20 to 100u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10100_200	100 to 200u particle size analysis, (method not recorded)
	P10200_600	200 to 600u particle size analysis, (method not recorded)
	P106002000	600 to 2000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded