Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1108	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	B. Purdie	Locality:
	Date Desc.:	22/04/98	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6513813 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	402068  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion:	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Parapanic Humic Aquic Podosol     	Principal Profile Form:	Uc1.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A1h	0 - 0.4 m	Black (2.5YR2/0-Moist); ; Sandy loam; Weak grade of structure, 50-100 mm, Platy; Moist; Weak 
	consistence; Field pH 4.3 (pH meter); Clear change to - 
	A21	0.4 - 0.6 m	Dark greyish brown (10YR4/2-Moist); ; Clayey sand; Single grain grade of structure; Moist; Very weak 
	consistence; Field pH 4.4 (pH meter); Clear change to - 
	A22	0.6 - 1.3 m	Greyish brown (10YR5/2-Moist); ; Clayey sand; Single grain grade of structure; Wet; Very weak 
	consistence; Field pH 4.9 (pH meter); Clear change to - 
	A23e	1.3 - 1.5 m	White (10YR8/1-Moist); ; Sand; Single grain grade of structure; Wet; Field pH 5.4 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Photos Roll 58-16/17. Cropping of hay.  Moist topsoil - humic. effective soil depth less due to high water table.

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1108	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.4	3.5B	12B	3.48H	2.33	0.12	0.95	0.28J	6.88D
	4.8H
	0.01 - 0.4	3.5B	12B	3.48H	2.33	0.12	0.95	0.28J	6.88D
	4.8H
	0.01 - 0.4	3.5B	12B	3.48H	2.33	0.12	0.95	0.28J	6.88D
	4.8H
	0.14 - 0.19
	0.4 - 0.6	3.6B	3B	0.07H	0.35	<0.02	0.1	0.05J	0.53D
	4.9H
	0.4 - 0.6	3.6B	3B	0.07H	0.35	<0.02	0.1	0.05J	0.53D
	4.9H
	0.4 - 0.6	3.6B	3B	0.07H	0.35	<0.02	0.1	0.05J	0.53D
	4.9H
	0.5 - 0.55
	0.6 - 1.3	4.2B	2B	0.1H	0.28	0.02	0.06	0.03J	0.46D
	5.6H
	0.6 - 1.3	4.2B	2B	0.1H	0.28	0.02	0.06	0.03J	0.46D
	5.6H
	0.6 - 1.3	4.2B	2B	0.1H	0.28	0.02	0.06	0.03J	0.46D
	5.6H
	1.3 - 1.5	4.8B	1B	<0.02K	0.03	<0.02	0.04	0.09D
	5.8H
	1.3 - 1.5	4.8B	1B	<0.02K	0.03	<0.02	0.04	0.09D
	5.8H
	1.3 - 1.5	4.8B	1B	<0.02K	0.03	<0.02	0.04	0.09D
	5.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.4	3.37D	41B	0.098E	4.4	3.2
	0.01 - 0.4	3.37D	41B	0.098E	4.4	3.2
	0.01 - 0.4	3.37D	41B	0.098E	4.4	3.2
	0.14 - 0.19	1.30
	0.4 - 0.6	0.59D	11B	0.008E	2.2	0.9
	0.4 - 0.6	0.59D	11B	0.008E	2.2	0.9
	0.4 - 0.6	0.59D	11B	0.008E	2.2	0.9
	0.5 - 0.55	1.60
	0.6 - 1.3	0.39D	12B	<0.005E	1.7	0.7
	0.6 - 1.3	0.39D	12B	<0.005E	1.7	0.7
	0.6 - 1.3	0.39D	12B	<0.005E	1.7	0.7
	1.3 - 1.5	0.05D	<10B	<0.005E	1.2	0.3
	1.3 - 1.5	0.05D	<10B	<0.005E	1.2	0.3
	1.3 - 1.5	0.05D	<10B	<0.005E	1.2	0.3
	Laboratory Analyses Completed for this profile
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1108	Observation 	1
	Agency Name:	Agriculture Western Australia
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_20_100	20 to 100u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10100_200	100 to 200u particle size analysis, (method not recorded)
	P10200_600	200 to 600u particle size analysis, (method not recorded)
	P106002000	600 to 2000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded