Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0185	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Bill Verboom	Locality:
	Date Desc.:	14/06/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6416337 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	622308  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Peneplain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 	; No surface coarse fragments
	Profile 
	A1	0 - 0.07 m	Brown (7.5YR4/4-Moist); , 0-0% ; Fine sandy loam; Weak grade of structure, <2 mm, Granular; 
	Moderately moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, subrounded, Ironstone, coarse 
	fragments; AbundantClear, Smooth change to - 
	A2c	0.07 - 0.2 m	Strong brown (7.5YR5/6-Moist); , 0-0% ; Fine sandy loam; Weak grade of structure, 2-5 mm; Moderately 
	moist; Weak consistence; 20-50%, medium gravelly, 6-20mm, subrounded, Ironstone, coarse fragments; 
	AbundantGradual, Wavy change to - 
	B2cw	0.2 - 0.3 m	Strong brown (7.5YR5/6-Moist); , 0-0% ; Fine sandy loam; Moderately moist; 20-50%, medium gravelly, 
	6-20mm, subrounded, Ironstone, coarse fragments; ManyGradual, Tongued change to - 
	B2cm	0.3 - 0.66 m	Red (2.5YR4/6-Moist); , 0-0% ; Sand; , Platy; Dry; Ferricrete, Massive; Few
	Morphological Notes
	A1	         
	A2c	Structure 2-5mm subrounded blocky.         
	B2cw	Gravelly         
	Observation Notes
	Site Notes
	Slight surface crust.    

	Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0185	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	5B	9B	4.36H	1.3	0.48	0.24	0.12J	6.38D
	5.6H
	0 - 0.07	5B	9B	4.36H	1.3	0.48	0.24	0.12J	6.38D
	5.6H
	0 - 0.04
	0.1 - 0.2	4B	10B	1.3H	0.65	0.13	0.22	1.09J	2.3D
	4.5H
	0.1 - 0.2	4B	10B	1.3H	0.65	0.13	0.22	1.09J	2.3D
	4.5H
	0.1 - 0.14
	0.2 - 0.3	3.9B	10B	0.98H	0.52	0.1	0.14	1.39J	1.74D
	4.3H
	0.2 - 0.3	3.9B	10B	0.98H	0.52	0.1	0.14	1.39J	1.74D
	4.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	1.76D	95B	0.085E	11	19.7
	0 - 0.07	1.76D	95B	0.085E	11	19.7
	0 - 0.04	1.44
	0.1 - 0.2	0.59D	48B	0.038E	7.7	32.2
	0.1 - 0.2	0.59D	48B	0.038E	7.7	32.2
	0.1 - 0.14	1.38
	0.2 - 0.3	43B	7.1	32.8
	0.2 - 0.3	43B	7.1	32.8
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)

	Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0185	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded