Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0188	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Bill Verboom	Locality:
	Date Desc.:	14/06/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6417360 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	622373  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 	; No surface coarse fragments
	Profile 
	A1	0 - 0.07 m	Dark greyish brown (2.5Y4/2-Moist); , 0-0% ; Fine sandy loam; Weak grade of structure, <2 mm, 
	Granular; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	AbundantClear, Smooth change to - 
	A2	0.07 - 0.3 m	Light brownish grey (2.5Y6/3-Moist); , 0-0% ; Fine sandy loam; Weak grade of structure, 2-5 mm, 
	Subangular blocky; Moderately moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; AbundantGradual, Smooth change to - 
	B2w	0.3 - 0.35 m	, 0-0% ; Moderately moist; Few
	B2w	0.35 - 0.5 m	Brownish yellow (10YR6/8-Moist); Mottles, 20-50% , 5-15mm, Prominent; Fine sandy loam; Massive 
	grade of structure; Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; Few
	Morphological Notes
	A1	         
	A2	         
	B2w	Gravel line above massive indurated mittle horizon.         
	B2w	         
	Observation Notes
	Site Notes
	Pale 20cm tall, 35cm wide,rounded termiteria.    

		Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0188	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	4.4B	2B	1.17H	0.25	0.12	0.06	0.37J	5.2C	1.6D	0.77
	5.5H	1.5F	0.4	0.04	0.04	1.98D
	4.3J
	0 - 0.07	4.4B	2B	1.17H	0.25	0.12	0.06	0.37J	5.2C	1.6D	0.77
	5.5H	1.5F	0.4	0.04	0.04	1.98D
	4.3J
	0 - 0.07	4.4B	2B	1.17H	0.25	0.12	0.06	0.37J	5.2C	1.6D	0.77
	5.5H	1.5F	0.4	0.04	0.04	1.98D
	4.3J
	0 - 0.04
	0.1 - 0.2	4.5B	2B	0.92H	0.52	0.14	0.09	0.18J	3.6C	1.67D	1.11
	5.5H	0.9F	0.6	0.04	0.04	1.58D
	4.4J
	0.1 - 0.2	4.5B	2B	0.92H	0.52	0.14	0.09	0.18J	3.6C	1.67D	1.11
	5.5H	0.9F	0.6	0.04	0.04	1.58D
	4.4J
	0.1 - 0.2	4.5B	2B	0.92H	0.52	0.14	0.09	0.18J	3.6C	1.67D	1.11
	5.5H	0.9F	0.6	0.04	0.04	1.58D
	4.4J
	0.13 - 0.17
	0.4 - 0.5	5.1B	3B	1.34H	2.38	0.06	0.15	0.02J	7.2C	3.93D	1.94
	5.6H	1.3F	2.2	0.02	0.14	3.66D
	4.9J
	0.4 - 0.5	5.1B	3B	1.34H	2.38	0.06	0.15	0.02J	7.2C	3.93D	1.94
	5.6H	1.3F	2.2	0.02	0.14	3.66D
	4.9J
	0.4 - 0.5	5.1B	3B	1.34H	2.38	0.06	0.15	0.02J	7.2C	3.93D	1.94
	5.6H	1.3F	2.2	0.02	0.14	3.66D
	4.9J
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	0.93D	28B	0.042E	19	4.3	10.9
	1.2A	5	8
	0 - 0.07	0.93D	28B	0.042E	19	4.3	10.9
	1.2A	5	8
	0 - 0.07	0.93D	28B	0.042E	19	4.3	10.9
	1.2A	5	8
	0 - 0.04	1.23
	0.1 - 0.2	0.33D	23B	0.026E	30	5.1	19.3
	0.41A	3	12
	0.1 - 0.2	0.33D	23B	0.026E	30	5.1	19.3
	0.41A	3	12
	0.1 - 0.2	0.33D	23B	0.026E	30	5.1	19.3
	0.41A	3	12
	0.13 - 0.17	1.28
	0.4 - 0.5	0.13A	33B	22	4.4	23
	7	16

	Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0188	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.4 - 0.5	0.13A	33B	22	4.4	23
	7	16
	0.4 - 0.5	0.13A	33B	22	4.4	23
	7	16
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15D1_AL	Exchangeable bases (Al2+)- 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1	Base saturation percentage (BSP)
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B_C_2.5	pH of soil - pH of 1:2.5 Soil/0.1M CaCl2 suspension
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10200_500	200 to 500u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P105002000	500 to 2000u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded

	Project Name:	Corrigin land resources survey
	Project Code:	COR	Site ID:	0188	Observation 	1
	Agency Name:	Agriculture Western Australia