Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0015	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Henry Smolinski	Locality:
	Date Desc.:	19/03/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6367690 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	424355  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	30 % 	Aspect:	90 degrees
	Surface Soil Condition 
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A11	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Loam; 2-5 mm, Granular; Moist; 20-50%, fine gravelly, 2-6mm, 
	subrounded, Ironstone, coarse fragments; Gradual, Wavy change to - 
	A12	0.1 - 0.4 m	Dark yellowish brown (10YR4/6-Moist); ; Sandy clay loam; 20-50 mm, ; Moderately moist; 20-50%, fine 
	gravelly, 2-6mm, subrounded, Ironstone, coarse fragments; Gradual, Wavy change to - 
	B2	0.4 - 0.9 m	Red (2.5YR4/6-Moist); ; Clay loam; 20-50 mm, Angular blocky; 2-5 mm, Polyhedral; Moderately moist; 
	20-50%, medium gravelly, 6-20mm, subrounded, Igneous rock (unidentified), coarse fragments; 10-20%, 
	fine gravelly, 2-6mm, rounded, Ironstone, coarse fragments; Clear, Irregular change to - 
	C	0.9 - 1.6 m	Reddish yellow (7.5YR6/8-Moist); , 5YR52, 10-20% , 0-5mm; Coarse sandy clay loam; 2-5 mm, Granular;
	 Moist; 10-20%, medium gravelly, 6-20mm, Igneous rock (unidentified), coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

		Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0015	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7B	4B	7.8A	3.02	0.39	0.18	11.39D
	6.7H
	0 - 0.1	5.7B	4B	7.8A	3.02	0.39	0.18	11.39D
	6.7H
	0.1 - 0.4	5.8B	2B	2.12A	1.39	0.27	0.09	3.87D
	7H
	0.1 - 0.4	5.8B	2B	2.12A	1.39	0.27	0.09	3.87D
	7H
	0.4 - 0.9	5.8B	2B	0.98A	0.93	0.28	0.1	2.29D
	6.7H
	0.4 - 0.9	5.8B	2B	0.98A	0.93	0.28	0.1	2.29D
	6.7H
	0.9 - 1.6	5.7B	2B	0.48H	0.92	0.11	0.12	1.63D
	6.2H
	0.9 - 1.6	5.7B	2B	0.48H	0.92	0.11	0.12	1.63D
	6.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	4.42D	180B	0.149E	11.9	10.9
	0 - 0.1	4.42D	180B	0.149E	11.9	10.9
	0.1 - 0.4	0.97D	100B	0.042E	9.9	22.6
	0.1 - 0.4	0.97D	100B	0.042E	9.9	22.6
	0.4 - 0.9	0.31D	94B	0.017E	9.3	28.4
	0.4 - 0.9	0.31D	94B	0.017E	9.3	28.4
	0.9 - 1.6	0.12D	74B	0.007E	9.2	26.7
	0.9 - 1.6	0.12D	74B	0.007E	9.2	26.7
	Laboratory Analyses Completed for this profile
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0015	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)